<?xml version="1.0" encoding="UTF-8" standalone="yes"?>
<topology xmlns="http://www.cisco.com/VIRL" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" schemaVersion="0.95" xsi:schemaLocation="http://www.cisco.com/VIRL https://raw.github.com/CiscoVIRL/schema/v0.95/virl.xsd">
    <extensions>
        <entry key="AutoNetkit.infrastructure_only" type="Boolean">false</entry>
        <entry key="management_network" type="String">flat</entry>
        <entry key="AutoNetkit.enable_cdp" type="Boolean">true</entry>
        <entry key="AutoNetkit.IGP" type="String">rip-v2</entry>
    </extensions>
    <node name="iosvl2-1" type="SIMPLE" subtype="IOSvL2" location="296,180">
        <extensions>
            <entry key="config" type="string">! IOSvL2 Config generated on 2017-08-27 14:56
! by autonetkit_0.23.5
!
version 15.2
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
service compress-config
no service config
enable password cisco
ip classless
ip subnet-zero
no ip domain lookup
!
line vty 0 4
transport input ssh telnet
exec-timeout 720 0
password cisco
login
!
line con 0
password cisco
!
hostname iosvl2-1
!
boot-start-marker
boot-end-marker
!
!
!
no aaa new-model
!
vtp domain virl.lab
vtp mode transparent
!
vlan 2
  name ank_vlan2
vlan 3
  name ank_vlan3
!
!
!
!
cdp run
!
!
!
ip cef
no ipv6 cef
!
!
spanning-tree mode pvst
spanning-tree extend system-id
!
vlan internal allocation policy ascending
!
!
!
!
vrf definition Mgmt-intf
!
 address-family ipv4
 exit-address-family
 !
 address-family ipv6
 exit-address-family
!
!
!
!
!
interface Loopback0
  description Loopback
!
interface GigabitEthernet0/0
  description OOB management
  ! Configured on launch
  no switchport
  vrf forwarding Mgmt-intf
  no ip address
  no shutdown
!
interface GigabitEthernet0/1
  description to iosvl2-2
  switchport trunk encapsulation dot1q
  switchport mode trunk
  no shutdown
!
interface GigabitEthernet0/2
  description to iosv-1
  switchport access vlan 2
  switchport mode access
  no shutdown
!
interface GigabitEthernet0/3
  description to kali-1
  switchport access vlan 2
  switchport mode access
  no shutdown
!
interface GigabitEthernet1/0
  description to iosv-2
  switchport access vlan 2
  switchport mode access
  no shutdown
!
!
ip forward-protocol nd
!
no ip http server
no ip http secure-server
!
!
!
!
!
!
control-plane
!
!
!
end
        </entry>
            <entry key="AutoNetkit.mgmt_ip" type="string"></entry>
        </extensions>
        <interface id="0" name="GigabitEthernet0/1"/>
        <interface id="1" name="GigabitEthernet0/2"/>
        <interface id="2" name="GigabitEthernet0/3"/>
        <interface id="3" name="GigabitEthernet1/0"/>
    </node>
    <node name="iosvl2-2" type="SIMPLE" subtype="IOSvL2" location="520,177">
        <extensions>
            <entry key="config" type="string">! IOSvL2 Config generated on 2017-08-27 14:56
! by autonetkit_0.23.5
!
version 15.2
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
service compress-config
no service config
enable password cisco
ip classless
ip subnet-zero
no ip domain lookup
!
line vty 0 4
transport input ssh telnet
exec-timeout 720 0
password cisco
login
!
line con 0
password cisco
!
hostname iosvl2-2
!
boot-start-marker
boot-end-marker
!
!
!
no aaa new-model
!
vtp domain virl.lab
vtp mode transparent
!
vlan 2
  name ank_vlan2
vlan 3
  name ank_vlan3
!
!
!
!
cdp run
!
!
!
ip cef
no ipv6 cef
!
!
spanning-tree mode pvst
spanning-tree extend system-id
!
vlan internal allocation policy ascending
!
!
!
!
vrf definition Mgmt-intf
!
 address-family ipv4
 exit-address-family
 !
 address-family ipv6
 exit-address-family
!
!
!
!
!
interface Loopback0
  description Loopback
!
interface GigabitEthernet0/0
  description OOB management
  ! Configured on launch
  no switchport
  vrf forwarding Mgmt-intf
  no ip address
  no shutdown
!
interface GigabitEthernet0/1
  description to iosvl2-1
  switchport trunk encapsulation dot1q
  switchport mode trunk
  no shutdown
!
interface GigabitEthernet0/2
  description to iosv-1
  switchport access vlan 3
  switchport mode access
  no shutdown
!
interface GigabitEthernet0/3
  description to server-1
  switchport access vlan 3
  switchport mode access
  no shutdown
!
!
ip forward-protocol nd
!
no ip http server
no ip http secure-server
!
!
!
!
!
!
control-plane
!
!
!
end
        </entry>
            <entry key="AutoNetkit.mgmt_ip" type="string"></entry>
        </extensions>
        <interface id="0" name="GigabitEthernet0/1"/>
        <interface id="1" name="GigabitEthernet0/2"/>
        <interface id="2" name="GigabitEthernet0/3"/>
    </node>
    <node name="kali-1" type="SIMPLE" subtype="kali" location="193,282">
        <extensions>
            <entry key="config" type="String">#cloud-config
bootcmd:
- ln -s -t /etc/rc.d /etc/rc.local
hostname: kali-1
manage_etc_hosts: true
package_update: true
packages:
- quagga
runcmd:
- start ttyS0
- systemctl start getty@ttyS0.service
- systemctl start rc-local
- sed -i '/^\s*PasswordAuthentication\s\+no/d' /etc/ssh/sshd_config
- echo "UseDNS no" &gt;&gt; /etc/ssh/sshd_config
- service ssh restart
- service sshd restart
users:
- default
- gecos: User configured by VIRL Configuration Engine 0.23.10
  lock-passwd: false
  name: cisco
  plain-text-passwd: cisco
  shell: /bin/bash
  ssh-authorized-keys:
  - VIRL-USER-SSH-PUBLIC-KEY
  sudo: ALL=(ALL) ALL
write_files:
- path: /etc/init/ttyS0.conf
  owner: root:root
  content: |
    # ttyS0 - getty
    # This service maintains a getty on ttyS0 from the point the system is
    # started until it is shut down again.
    start on stopped rc or RUNLEVEL=[12345]
    stop on runlevel [!12345]
    respawn
    exec /sbin/getty -L 115200 ttyS0 vt102
  permissions: '0644'
- path: /etc/systemd/system/dhclient@.service
  content: |
    [Unit]
    Description=Run dhclient on %i interface
    After=network.target
    [Service]
    Type=oneshot
    ExecStart=/sbin/dhclient %i -pf /var/run/dhclient.%i.pid -lf /var/lib/dhclient/dhclient.%i.lease
    RemainAfterExit=yes
  owner: root:root
  permissions: '0644'
- path: /etc/rc.local
  owner: root:root
  permissions: '0755'
  content: |-
    #!/bin/sh
    ip route del default
    ip route add default via 172.16.1.2
    ip link set eth1 up
    ip addr add 10.0.0.1/17 dev eth1
    # Use routes from Quagga instead
    #route add -host 192.168.0.1 gw 10.0.0.2 dev eth1
    #route add -host 192.168.0.4 gw 10.0.0.2 dev eth1
    #route add -net 10.0.0.0/17 gw 10.0.0.2 dev eth1
    #route add -net 10.0.128.0/30 gw 10.0.0.2 dev eth1
    #route add -host 192.168.0.1 gw 10.0.0.3 dev eth1
    #route add -host 192.168.0.4 gw 10.0.0.3 dev eth1
    #route add -net 10.0.0.0/17 gw 10.0.0.3 dev eth1
    #route add -net 10.0.128.0/30 gw 10.0.0.3 dev eth1
    exit 0
- path: /etc/quagga/zebra.conf
  owner: root:root
  permissions: '0644'
  content: |-
    hostname kali-1
    password cisco
    enable password cisco
    interface eth0
    interface eth1
    line vty
- path: /etc/quagga/ripd.conf
  owner: root:root
  permissions: '0644'
  content: |-
    hostname kali-1
    password cisco
    log stdout
    router rip
      network eth1
    line vty
</entry>
        </extensions>
        <interface id="0" name="eth1" ipv4="10.0.0.1" netPrefixLenV4="17">
            <extensions>
                <entry key="AutoNetkit.vlan" type="Integer">2</entry>
            </extensions>
        </interface>
    </node>
    <node name="iosv-1" type="SIMPLE" subtype="IOSv" location="417,76" ipv4="192.168.0.1">
        <extensions>
            <entry key="config" type="string">! IOS Config generated on 2017-08-27 14:56
! by autonetkit_0.23.5
!
hostname iosv-1
boot-start-marker
boot-end-marker
!
vrf definition Mgmt-intf
!
 address-family ipv4
 exit-address-family
 !
 address-family ipv6
 exit-address-family
!
!
!
no aaa new-model
!
!
ip cef
ipv6 unicast-routing
ipv6 cef
!
!
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
no service config
enable password cisco
ip classless
ip subnet-zero
no ip domain lookup
ip domain name virl.info
crypto key generate rsa modulus 768
ip ssh server algorithm authentication password
username cisco privilege 15 secret cisco
line vty 0 4
 transport input ssh telnet
 exec-timeout 720 0
 password cisco
 login local
line con 0
 password cisco
!
cdp run
!
!
interface Loopback0
  description Loopback
  ip address 192.168.0.1 255.255.255.255
!
interface GigabitEthernet0/0
  description OOB Management
  vrf forwarding Mgmt-intf
  ! Configured on launch
  no ip address
  cdp enable
  duplex full
  speed auto
  no shutdown
!
interface GigabitEthernet0/1
  description to iosvl2-1
  ip address 10.0.0.2 255.255.128.0
  cdp enable
  duplex full
  speed auto
  no shutdown
!
interface GigabitEthernet0/2
  description to iosvl2-2
  ip address 10.0.128.1 255.255.255.252
  cdp enable
  duplex full
  speed auto
  no shutdown
!
!
!
router rip
  version 2
  no auto-summary
  network 10.0.0.0
  network 10.0.128.0
  network 192.168.0.1
  passive-interface GigabitEthernet0/0
!
!
router bgp 1
  bgp router-id 192.168.0.1
  no synchronization
! ibgp
  ! ibgp peers
  !
  neighbor 192.168.0.4 remote-as 1
  neighbor 192.168.0.4 description iBGP peer iosv-2
  neighbor 192.168.0.4 update-source Loopback0
!
!
 !
 address-family ipv4
  network 192.168.0.1 mask 255.255.255.255
  neighbor 192.168.0.4 activate
 exit-address-family
!
!
!
end</entry>
            <entry key="AutoNetkit.mgmt_ip" type="string"></entry>
        </extensions>
        <interface id="0" name="GigabitEthernet0/1" ipv4="10.0.0.2" netPrefixLenV4="17">
            <extensions>
                <entry key="AutoNetkit.vlan" type="Integer">2</entry>
            </extensions>
        </interface>
        <interface id="1" name="GigabitEthernet0/2" ipv4="10.0.128.1" netPrefixLenV4="30">
            <extensions>
                <entry key="AutoNetkit.vlan" type="Integer">3</entry>
            </extensions>
        </interface>
    </node>
    <node name="server-1" type="SIMPLE" subtype="server" location="592,287">
        <extensions>
            <entry key="config" type="string">#cloud-config
bootcmd:
- ln -s -t /etc/rc.d /etc/rc.local
hostname: server-1
manage_etc_hosts: true
runcmd:
- start ttyS0
- systemctl start getty@ttyS0.service
- systemctl start rc-local
- sed -i '/^\s*PasswordAuthentication\s\+no/d' /etc/ssh/sshd_config
- echo "UseDNS no" &gt;&gt; /etc/ssh/sshd_config
- service ssh restart
- service sshd restart
users:
- default
- gecos: User configured by VIRL Configuration Engine 0.23.10
  lock-passwd: false
  name: cisco
  plain-text-passwd: cisco
  shell: /bin/bash
  ssh-authorized-keys:
  - VIRL-USER-SSH-PUBLIC-KEY
  sudo: ALL=(ALL) ALL
write_files:
- path: /etc/init/ttyS0.conf
  owner: root:root
  content: |
    # ttyS0 - getty
    # This service maintains a getty on ttyS0 from the point the system is
    # started until it is shut down again.
    start on stopped rc or RUNLEVEL=[12345]
    stop on runlevel [!12345]
    respawn
    exec /sbin/getty -L 115200 ttyS0 vt102
  permissions: '0644'
- path: /etc/systemd/system/dhclient@.service
  content: |
    [Unit]
    Description=Run dhclient on %i interface
    After=network.target
    [Service]
    Type=oneshot
    ExecStart=/sbin/dhclient %i -pf /var/run/dhclient.%i.pid -lf /var/lib/dhclient/dhclient.%i.lease
    RemainAfterExit=yes
  owner: root:root
  permissions: '0644'
- path: /etc/rc.local
  owner: root:root
  permissions: '0755'
  content: |-
    #!/bin/sh
    ifconfig eth1 up 10.0.128.2 netmask 255.255.255.252
    route add -host 192.168.0.1 gw 10.0.128.1 dev eth1
    route add -host 192.168.0.4 gw 10.0.128.1 dev eth1
    route add -net 10.0.0.0/17 gw 10.0.128.1 dev eth1
    route add -net 10.0.128.0/30 gw 10.0.128.1 dev eth1
    exit 0
</entry>
        </extensions>
        <interface id="0" name="eth1" ipv4="10.0.128.2" netPrefixLenV4="30">
            <extensions>
                <entry key="AutoNetkit.vlan" type="Integer">3</entry>
            </extensions>
        </interface>
    </node>
    <node name="iosv-2" type="SIMPLE" subtype="IOSv" location="370,291" ipv4="192.168.0.4">
        <extensions>
            <entry key="AutoNetkit.mgmt_ip" type="string"></entry>
            <entry key="config" type="String">! IOS Config generated on 2017-08-27 14:56
! by autonetkit_0.23.5
!
hostname iosv-2
boot-start-marker
boot-end-marker
!
vrf definition Mgmt-intf
!
 address-family ipv4
 exit-address-family
 !
 address-family ipv6
 exit-address-family
!
!
!
no aaa new-model
!
!
ip cef
ipv6 unicast-routing
ipv6 cef
!
!
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
no service config
enable password cisco
ip classless
ip subnet-zero
no ip domain lookup
ip domain name virl.info
crypto key generate rsa modulus 768
ip ssh server algorithm authentication password
username cisco privilege 15 secret cisco
ip access-list standard IN-VTY
  permit 172.16.1.0 0.0.0.255
  permit 192.168.0.0 0.0.0.255
  permit 10.0.128.0 0.0.0.3
line vty 0 4
 transport input ssh telnet
 access-class IN-VTY in vrf-also
 exec-timeout 720 0
 password cisco
 login local
line con 0
 password cisco
!
cdp run
!
!
interface Loopback0
  description Loopback
  ip address 192.168.0.4 255.255.255.255
!
interface GigabitEthernet0/0
  description OOB Management
  vrf forwarding Mgmt-intf
  ! Configured on launch
  no ip address
  cdp enable
  duplex full
  speed auto
  no shutdown
!
interface GigabitEthernet0/1
  description to iosvl2-1
  ip address 10.0.0.3 255.255.128.0
  cdp enable
  duplex full
  speed auto
  no shutdown
!
!
!
router rip
  version 2
  no auto-summary
  network 10.0.0.0
  network 192.168.0.4
  passive-interface GigabitEthernet0/0
!
!
router bgp 1
  bgp router-id 192.168.0.4
  no synchronization
! ibgp
  ! ibgp peers
  !
  neighbor 192.168.0.1 remote-as 1
  neighbor 192.168.0.1 description iBGP peer iosv-1
  neighbor 192.168.0.1 update-source Loopback0
!
!
 !
 address-family ipv4
  network 192.168.0.4 mask 255.255.255.255
  neighbor 192.168.0.1 activate
 exit-address-family
!
!
!
end</entry>
        </extensions>
        <interface id="0" name="GigabitEthernet0/1" ipv4="10.0.0.3" netPrefixLenV4="17">
            <extensions>
                <entry key="AutoNetkit.vlan" type="Integer">2</entry>
            </extensions>
        </interface>
    </node>
    <annotations/>
    <connection dst="/virl:topology/virl:node[2]/virl:interface[1]" src="/virl:topology/virl:node[1]/virl:interface[1]"/>
    <connection dst="/virl:topology/virl:node[1]/virl:interface[2]" src="/virl:topology/virl:node[4]/virl:interface[1]"/>
    <connection dst="/virl:topology/virl:node[4]/virl:interface[2]" src="/virl:topology/virl:node[2]/virl:interface[2]"/>
    <connection dst="/virl:topology/virl:node[1]/virl:interface[3]" src="/virl:topology/virl:node[3]/virl:interface[1]"/>
    <connection dst="/virl:topology/virl:node[2]/virl:interface[3]" src="/virl:topology/virl:node[5]/virl:interface[1]"/>
    <connection dst="/virl:topology/virl:node[6]/virl:interface[1]" src="/virl:topology/virl:node[1]/virl:interface[4]"/>
</topology>
