<?xml version="1.0" encoding="UTF-8" standalone="yes"?>
<topology xmlns="http://www.cisco.com/VIRL" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" schemaVersion="0.95" xsi:schemaLocation="http://www.cisco.com/VIRL https://raw.github.com/CiscoVIRL/schema/v0.95/virl.xsd">
    <node name="iosv-1" type="SIMPLE" subtype="IOSv" location="301,221" ipv4="192.168.0.3">
        <extensions>
            <entry key="config" type="string">! IOS Config generated on 2018-06-02 05:15
! by autonetkit_0.24.0
!
hostname iosv-1
boot-start-marker
boot-end-marker
!
vrf definition Mgmt-intf
!
 address-family ipv4
 exit-address-family
 !
 address-family ipv6
 exit-address-family
!
!
!
no aaa new-model
!
!
ip cef
ipv6 unicast-routing
ipv6 cef
!
!
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
no service config
enable password cisco
ip classless
ip subnet-zero
no ip domain lookup
ip domain name virl.info
crypto key generate rsa modulus 768
ip ssh server algorithm authentication password
username cisco privilege 15 secret cisco
line vty 0 4
 transport input ssh telnet
 exec-timeout 720 0
 password cisco
 login local
line con 0
 password cisco
!
no cdp run
!
!
interface Loopback0
  description Loopback
  ip address 192.168.0.3 255.255.255.255
!
interface GigabitEthernet0/0
  description OOB Management
  vrf forwarding Mgmt-intf
  ! Configured on launch
  no ip address
  duplex full
  speed auto
  no shutdown
!
interface GigabitEthernet0/1
  description to server-1
  ip address 10.0.0.5 255.255.255.252
  ip ospf cost 1
  duplex full
  speed auto
  no shutdown
!
interface GigabitEthernet0/2
  description to iosv-4
  ip address 10.0.0.17 255.255.255.252
  ip ospf cost 1
  duplex full
  speed auto
  no shutdown
!
!
!
router ospf 1
  network 192.168.0.3 0.0.0.0 area 0
  log-adjacency-changes
  passive-interface Loopback0
  network 10.0.0.4 0.0.0.3 area 0
  network 10.0.0.16 0.0.0.3 area 0
!
!
router bgp 1
  bgp router-id 192.168.0.3
  no synchronization
! ibgp
  ! ibgp peers
  !
  neighbor 192.168.0.4 remote-as 1
  neighbor 192.168.0.4 description iBGP peer iosv-2
  neighbor 192.168.0.4 update-source Loopback0
  !
  neighbor 192.168.0.7 remote-as 1
  neighbor 192.168.0.7 description iBGP peer iosv-3
  neighbor 192.168.0.7 update-source Loopback0
  !
  neighbor 192.168.0.8 remote-as 1
  neighbor 192.168.0.8 description iBGP peer iosv-4
  neighbor 192.168.0.8 update-source Loopback0
!
!
 !
 address-family ipv4
  network 192.168.0.3 mask 255.255.255.255
  neighbor 192.168.0.4 activate
  neighbor 192.168.0.7 activate
  neighbor 192.168.0.8 activate
 exit-address-family
!
!
!
end</entry>
            <entry key="AutoNetkit.mgmt_ip" type="string"></entry>
        </extensions>
        <interface id="0" name="GigabitEthernet0/1" ipv4="10.0.0.5" netPrefixLenV4="30"/>
        <interface id="1" name="GigabitEthernet0/2" ipv4="10.0.0.17" netPrefixLenV4="30"/>
    </node>
    <node name="iosv-2" type="SIMPLE" subtype="IOSv" location="306,368" ipv4="192.168.0.4">
        <extensions>
            <entry key="config" type="string">! IOS Config generated on 2018-06-02 05:15
! by autonetkit_0.24.0
!
hostname iosv-2
boot-start-marker
boot-end-marker
!
vrf definition Mgmt-intf
!
 address-family ipv4
 exit-address-family
 !
 address-family ipv6
 exit-address-family
!
!
!
no aaa new-model
!
!
ip cef
ipv6 unicast-routing
ipv6 cef
!
!
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
no service config
enable password cisco
ip classless
ip subnet-zero
no ip domain lookup
ip domain name virl.info
crypto key generate rsa modulus 768
ip ssh server algorithm authentication password
username cisco privilege 15 secret cisco
line vty 0 4
 transport input ssh telnet
 exec-timeout 720 0
 password cisco
 login local
line con 0
 password cisco
!
no cdp run
!
!
interface Loopback0
  description Loopback
  ip address 192.168.0.4 255.255.255.255
!
interface GigabitEthernet0/0
  description OOB Management
  vrf forwarding Mgmt-intf
  ! Configured on launch
  no ip address
  duplex full
  speed auto
  no shutdown
!
interface GigabitEthernet0/1
  description to server-2
  ip address 10.0.0.21 255.255.255.252
  ip ospf cost 1
  duplex full
  speed auto
  no shutdown
!
interface GigabitEthernet0/2
  description to iosv-4
  ip address 10.0.0.25 255.255.255.252
  ip ospf cost 1
  duplex full
  speed auto
  no shutdown
!
!
!
router ospf 1
  network 192.168.0.4 0.0.0.0 area 0
  log-adjacency-changes
  passive-interface Loopback0
  network 10.0.0.20 0.0.0.3 area 0
  network 10.0.0.24 0.0.0.3 area 0
!
!
router bgp 1
  bgp router-id 192.168.0.4
  no synchronization
! ibgp
  ! ibgp peers
  !
  neighbor 192.168.0.3 remote-as 1
  neighbor 192.168.0.3 description iBGP peer iosv-1
  neighbor 192.168.0.3 update-source Loopback0
  !
  neighbor 192.168.0.7 remote-as 1
  neighbor 192.168.0.7 description iBGP peer iosv-3
  neighbor 192.168.0.7 update-source Loopback0
  !
  neighbor 192.168.0.8 remote-as 1
  neighbor 192.168.0.8 description iBGP peer iosv-4
  neighbor 192.168.0.8 update-source Loopback0
!
!
 !
 address-family ipv4
  network 192.168.0.4 mask 255.255.255.255
  neighbor 192.168.0.3 activate
  neighbor 192.168.0.7 activate
  neighbor 192.168.0.8 activate
 exit-address-family
!
!
!
end</entry>
            <entry key="AutoNetkit.mgmt_ip" type="string"></entry>
        </extensions>
        <interface id="0" name="GigabitEthernet0/1" ipv4="10.0.0.21" netPrefixLenV4="30"/>
        <interface id="1" name="GigabitEthernet0/2" ipv4="10.0.0.25" netPrefixLenV4="30"/>
    </node>
    <node name="iosv-3" type="SIMPLE" subtype="IOSv" location="678,276" ipv4="192.168.0.7">
        <extensions>
            <entry key="config" type="string">! IOS Config generated on 2018-06-02 05:15
! by autonetkit_0.24.0
!
hostname iosv-3
boot-start-marker
boot-end-marker
!
vrf definition Mgmt-intf
!
 address-family ipv4
 exit-address-family
 !
 address-family ipv6
 exit-address-family
!
!
!
no aaa new-model
!
!
ip cef
ipv6 unicast-routing
ipv6 cef
!
!
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
no service config
enable password cisco
ip classless
ip subnet-zero
no ip domain lookup
ip domain name virl.info
crypto key generate rsa modulus 768
ip ssh server algorithm authentication password
username cisco privilege 15 secret cisco
line vty 0 4
 transport input ssh telnet
 exec-timeout 720 0
 password cisco
 login local
line con 0
 password cisco
!
no cdp run
!
!
interface Loopback0
  description Loopback
  ip address 192.168.0.7 255.255.255.255
!
interface GigabitEthernet0/0
  description OOB Management
  vrf forwarding Mgmt-intf
  ! Configured on launch
  no ip address
  duplex full
  speed auto
  no shutdown
!
interface GigabitEthernet0/1
  description to asav-1
  ip address 10.0.0.10 255.255.255.252
  ip ospf cost 1
  duplex full
  speed auto
  no shutdown
!
interface GigabitEthernet0/2
  description to server-3
  ip address 10.0.0.29 255.255.255.252
  ip ospf cost 1
  duplex full
  speed auto
  no shutdown
!
!
!
router ospf 1
  network 192.168.0.7 0.0.0.0 area 0
  log-adjacency-changes
  passive-interface Loopback0
  network 10.0.0.8 0.0.0.3 area 0
  network 10.0.0.28 0.0.0.3 area 0
!
!
router bgp 1
  bgp router-id 192.168.0.7
  no synchronization
! ibgp
  ! ibgp peers
  !
  neighbor 192.168.0.3 remote-as 1
  neighbor 192.168.0.3 description iBGP peer iosv-1
  neighbor 192.168.0.3 update-source Loopback0
  !
  neighbor 192.168.0.4 remote-as 1
  neighbor 192.168.0.4 description iBGP peer iosv-2
  neighbor 192.168.0.4 update-source Loopback0
  !
  neighbor 192.168.0.8 remote-as 1
  neighbor 192.168.0.8 description iBGP peer iosv-4
  neighbor 192.168.0.8 update-source Loopback0
!
!
 !
 address-family ipv4
  network 192.168.0.7 mask 255.255.255.255
  neighbor 192.168.0.3 activate
  neighbor 192.168.0.4 activate
  neighbor 192.168.0.8 activate
 exit-address-family
!
!
!
end</entry>
            <entry key="AutoNetkit.mgmt_ip" type="string"></entry>
        </extensions>
        <interface id="0" name="GigabitEthernet0/1" ipv4="10.0.0.10" netPrefixLenV4="30"/>
        <interface id="1" name="GigabitEthernet0/2" ipv4="10.0.0.29" netPrefixLenV4="30"/>
    </node>
    <node name="asav-1" type="SIMPLE" subtype="ASAv" location="543,274">
        <extensions>
            <entry key="config" type="string">! ASAv Config generated on 2018-06-02 05:15
! by autonetkit_0.24.0
!
hostname asav-1
username cisco password cisco privilege 15
enable password cisco
passwd cisco
names
!
interface GigabitEthernet0/0
  description to iosv-4
  duplex full
  nameif outside
  security-level 0
  no shutdown
  ip address 10.0.0.13 255.255.255.252
interface GigabitEthernet0/1
  description to iosv-3
  duplex full
  nameif outside-1
  security-level 0
  no shutdown
  ip address 10.0.0.9 255.255.255.252
interface Management0/0
  description OOB Management
  duplex full
  management-only
  nameif mgmt
  security-level 100
  no shutdown
  ! Configured on launch
  no ip address
!
same-security-traffic permit inter-interface
logging enable
logging asdm informational
user-identity default-domain LOCAL
aaa authentication ssh console LOCAL
http server enable
http 0.0.0.0 0.0.0.0 mgmt
ssh 0.0.0.0 0.0.0.0 mgmt
telnet 0.0.0.0 0.0.0.0 mgmt
http 0.0.0.0 0.0.0.0 outside
ssh 0.0.0.0 0.0.0.0 outside
telnet 0.0.0.0 0.0.0.0 outside
http 0.0.0.0 0.0.0.0 outside-1
ssh 0.0.0.0 0.0.0.0 outside-1
telnet 0.0.0.0 0.0.0.0 outside-1
ssh version 2
crypto key generate rsa modulus 768
telnet timeout 15
console timeout 0
username cisco password cisco privilege 15
!
class-map inspection_default
 match default-inspection-traffic
!
!
policy-map type inspect dns preset_dns_map
 parameters
  message-length maximum client auto
  message-length maximum 512
policy-map global_policy
 class inspection_default
  inspect ip-options
  inspect netbios
  inspect rtsp
  inspect sunrpc
  inspect tftp
  inspect xdmcp
  inspect dns preset_dns_map
  inspect ftp
  inspect h323 h225
  inspect h323 ras
  inspect rsh
  inspect esmtp
  inspect sqlnet
  inspect sip
  inspect skinny
  inspect icmp
  inspect http
!
service-policy global_policy global
no call-home reporting anonymous
call-home
 profile CiscoTAC-1
  no active
end
        </entry>
            <entry key="AutoNetkit.mgmt_ip" type="string"></entry>
        </extensions>
        <interface id="0" name="GigabitEthernet0/0" ipv4="10.0.0.13" netPrefixLenV4="30"/>
        <interface id="1" name="GigabitEthernet0/1" ipv4="10.0.0.9" netPrefixLenV4="30"/>
    </node>
    <node name="server-1" type="SIMPLE" subtype="server" location="181,216">
        <extensions>
            <entry key="config" type="string">#cloud-config
bootcmd:
- ln -s -t /etc/rc.d /etc/rc.local
hostname: server-1
manage_etc_hosts: true
runcmd:
- start ttyS0
- systemctl start getty@ttyS0.service
- systemctl start rc-local
- sed -i '/^\s*PasswordAuthentication\s\+no/d' /etc/ssh/sshd_config
- echo "UseDNS no" &gt;&gt; /etc/ssh/sshd_config
- service ssh restart
- service sshd restart
users:
- default
- gecos: User configured by VIRL Configuration Engine 0.23.10
  lock-passwd: false
  name: cisco
  plain-text-passwd: cisco
  shell: /bin/bash
  ssh-authorized-keys:
  - VIRL-USER-SSH-PUBLIC-KEY
  sudo: ALL=(ALL) ALL
write_files:
- path: /etc/init/ttyS0.conf
  owner: root:root
  content: |
    # ttyS0 - getty
    # This service maintains a getty on ttyS0 from the point the system is
    # started until it is shut down again.
    start on stopped rc or RUNLEVEL=[12345]
    stop on runlevel [!12345]
    respawn
    exec /sbin/getty -L 115200 ttyS0 vt102
  permissions: '0644'
- path: /etc/systemd/system/dhclient@.service
  content: |
    [Unit]
    Description=Run dhclient on %i interface
    After=network.target
    [Service]
    Type=oneshot
    ExecStart=/sbin/dhclient %i -pf /var/run/dhclient.%i.pid -lf /var/lib/dhclient/dhclient.%i.lease
    RemainAfterExit=yes
  owner: root:root
  permissions: '0644'
- path: /etc/rc.local
  owner: root:root
  permissions: '0755'
  content: |-
    #!/bin/sh
    ifconfig eth1 up 10.0.0.6 netmask 255.255.255.252
    route add -net 10.0.0.0/8 gw 10.0.0.5 dev eth1
    route add -net 192.168.0.0/28 gw 10.0.0.5 dev eth1
    exit 0
</entry>
        </extensions>
        <interface id="0" name="eth1" ipv4="10.0.0.6" netPrefixLenV4="30"/>
    </node>
    <node name="server-2" type="SIMPLE" subtype="server" location="178,366">
        <extensions>
            <entry key="config" type="string">#cloud-config
bootcmd:
- ln -s -t /etc/rc.d /etc/rc.local
hostname: server-2
manage_etc_hosts: true
runcmd:
- start ttyS0
- systemctl start getty@ttyS0.service
- systemctl start rc-local
- sed -i '/^\s*PasswordAuthentication\s\+no/d' /etc/ssh/sshd_config
- echo "UseDNS no" &gt;&gt; /etc/ssh/sshd_config
- service ssh restart
- service sshd restart
users:
- default
- gecos: User configured by VIRL Configuration Engine 0.23.10
  lock-passwd: false
  name: cisco
  plain-text-passwd: cisco
  shell: /bin/bash
  ssh-authorized-keys:
  - VIRL-USER-SSH-PUBLIC-KEY
  sudo: ALL=(ALL) ALL
write_files:
- path: /etc/init/ttyS0.conf
  owner: root:root
  content: |
    # ttyS0 - getty
    # This service maintains a getty on ttyS0 from the point the system is
    # started until it is shut down again.
    start on stopped rc or RUNLEVEL=[12345]
    stop on runlevel [!12345]
    respawn
    exec /sbin/getty -L 115200 ttyS0 vt102
  permissions: '0644'
- path: /etc/systemd/system/dhclient@.service
  content: |
    [Unit]
    Description=Run dhclient on %i interface
    After=network.target
    [Service]
    Type=oneshot
    ExecStart=/sbin/dhclient %i -pf /var/run/dhclient.%i.pid -lf /var/lib/dhclient/dhclient.%i.lease
    RemainAfterExit=yes
  owner: root:root
  permissions: '0644'
- path: /etc/rc.local
  owner: root:root
  permissions: '0755'
  content: |-
    #!/bin/sh
    ifconfig eth1 up 10.0.0.22 netmask 255.255.255.252
    route add -net 10.0.0.0/8 gw 10.0.0.21 dev eth1
    route add -net 192.168.0.0/28 gw 10.0.0.21 dev eth1
    exit 0
</entry>
        </extensions>
        <interface id="0" name="eth1" ipv4="10.0.0.22" netPrefixLenV4="30"/>
    </node>
    <node name="server-3" type="SIMPLE" subtype="server" location="809,276">
        <extensions>
            <entry key="config" type="string">#cloud-config
bootcmd:
- ln -s -t /etc/rc.d /etc/rc.local
hostname: server-3
manage_etc_hosts: true
runcmd:
- start ttyS0
- systemctl start getty@ttyS0.service
- systemctl start rc-local
- sed -i '/^\s*PasswordAuthentication\s\+no/d' /etc/ssh/sshd_config
- echo "UseDNS no" &gt;&gt; /etc/ssh/sshd_config
- service ssh restart
- service sshd restart
users:
- default
- gecos: User configured by VIRL Configuration Engine 0.23.10
  lock-passwd: false
  name: cisco
  plain-text-passwd: cisco
  shell: /bin/bash
  ssh-authorized-keys:
  - VIRL-USER-SSH-PUBLIC-KEY
  sudo: ALL=(ALL) ALL
write_files:
- path: /etc/init/ttyS0.conf
  owner: root:root
  content: |
    # ttyS0 - getty
    # This service maintains a getty on ttyS0 from the point the system is
    # started until it is shut down again.
    start on stopped rc or RUNLEVEL=[12345]
    stop on runlevel [!12345]
    respawn
    exec /sbin/getty -L 115200 ttyS0 vt102
  permissions: '0644'
- path: /etc/systemd/system/dhclient@.service
  content: |
    [Unit]
    Description=Run dhclient on %i interface
    After=network.target
    [Service]
    Type=oneshot
    ExecStart=/sbin/dhclient %i -pf /var/run/dhclient.%i.pid -lf /var/lib/dhclient/dhclient.%i.lease
    RemainAfterExit=yes
  owner: root:root
  permissions: '0644'
- path: /etc/rc.local
  owner: root:root
  permissions: '0755'
  content: |-
    #!/bin/sh
    ifconfig eth1 up 10.0.0.30 netmask 255.255.255.252
    route add -net 10.0.0.0/8 gw 10.0.0.29 dev eth1
    route add -net 192.168.0.0/28 gw 10.0.0.29 dev eth1
    exit 0
</entry>
        </extensions>
        <interface id="0" name="eth1" ipv4="10.0.0.30" netPrefixLenV4="30"/>
    </node>
    <node name="iosv-4" type="SIMPLE" subtype="IOSv" location="428,272" ipv4="192.168.0.8">
        <extensions>
            <entry key="config" type="string">! IOS Config generated on 2018-06-02 05:15
! by autonetkit_0.24.0
!
hostname iosv-4
boot-start-marker
boot-end-marker
!
vrf definition Mgmt-intf
!
 address-family ipv4
 exit-address-family
 !
 address-family ipv6
 exit-address-family
!
!
!
no aaa new-model
!
!
ip cef
ipv6 unicast-routing
ipv6 cef
!
!
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
no service config
enable password cisco
ip classless
ip subnet-zero
no ip domain lookup
ip domain name virl.info
crypto key generate rsa modulus 768
ip ssh server algorithm authentication password
username cisco privilege 15 secret cisco
line vty 0 4
 transport input ssh telnet
 exec-timeout 720 0
 password cisco
 login local
line con 0
 password cisco
!
no cdp run
!
!
interface Loopback0
  description Loopback
  ip address 192.168.0.8 255.255.255.255
!
interface GigabitEthernet0/0
  description OOB Management
  vrf forwarding Mgmt-intf
  ! Configured on launch
  no ip address
  duplex full
  speed auto
  no shutdown
!
interface GigabitEthernet0/1
  description to iosv-1
  ip address 10.0.0.18 255.255.255.252
  ip ospf cost 1
  duplex full
  speed auto
  no shutdown
!
interface GigabitEthernet0/2
  description to iosv-2
  ip address 10.0.0.26 255.255.255.252
  ip ospf cost 1
  duplex full
  speed auto
  no shutdown
!
interface GigabitEthernet0/3
  description to asav-1
  ip address 10.0.0.14 255.255.255.252
  ip ospf cost 1
  duplex full
  speed auto
  no shutdown
!
!
!
router ospf 1
  network 192.168.0.8 0.0.0.0 area 0
  log-adjacency-changes
  passive-interface Loopback0
  network 10.0.0.16 0.0.0.3 area 0
  network 10.0.0.24 0.0.0.3 area 0
  network 10.0.0.12 0.0.0.3 area 0
!
!
router bgp 1
  bgp router-id 192.168.0.8
  no synchronization
! ibgp
  ! ibgp peers
  !
  neighbor 192.168.0.3 remote-as 1
  neighbor 192.168.0.3 description iBGP peer iosv-1
  neighbor 192.168.0.3 update-source Loopback0
  !
  neighbor 192.168.0.4 remote-as 1
  neighbor 192.168.0.4 description iBGP peer iosv-2
  neighbor 192.168.0.4 update-source Loopback0
  !
  neighbor 192.168.0.7 remote-as 1
  neighbor 192.168.0.7 description iBGP peer iosv-3
  neighbor 192.168.0.7 update-source Loopback0
!
!
 !
 address-family ipv4
  network 192.168.0.8 mask 255.255.255.255
  neighbor 192.168.0.3 activate
  neighbor 192.168.0.4 activate
  neighbor 192.168.0.7 activate
 exit-address-family
!
!
!
end</entry>
            <entry key="AutoNetkit.mgmt_ip" type="string"></entry>
        </extensions>
        <interface id="0" name="GigabitEthernet0/1" ipv4="10.0.0.18" netPrefixLenV4="30"/>
        <interface id="1" name="GigabitEthernet0/2" ipv4="10.0.0.26" netPrefixLenV4="30"/>
        <interface id="2" name="GigabitEthernet0/3" ipv4="10.0.0.14" netPrefixLenV4="30"/>
    </node>
    <annotations/>
    <connection dst="/virl:topology/virl:node[1]/virl:interface[1]" src="/virl:topology/virl:node[5]/virl:interface[1]"/>
    <connection dst="/virl:topology/virl:node[2]/virl:interface[1]" src="/virl:topology/virl:node[6]/virl:interface[1]"/>
    <connection dst="/virl:topology/virl:node[8]/virl:interface[1]" src="/virl:topology/virl:node[1]/virl:interface[2]"/>
    <connection dst="/virl:topology/virl:node[8]/virl:interface[2]" src="/virl:topology/virl:node[2]/virl:interface[2]"/>
    <connection dst="/virl:topology/virl:node[4]/virl:interface[1]" src="/virl:topology/virl:node[8]/virl:interface[3]"/>
    <connection dst="/virl:topology/virl:node[3]/virl:interface[1]" src="/virl:topology/virl:node[4]/virl:interface[2]"/>
    <connection dst="/virl:topology/virl:node[7]/virl:interface[1]" src="/virl:topology/virl:node[3]/virl:interface[2]"/>
</topology>
