<?xml version="1.0" encoding="UTF-8" standalone="yes"?>
<topology xmlns="http://www.cisco.com/VIRL" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" schemaVersion="0.95" xsi:schemaLocation="http://www.cisco.com/VIRL https://raw.github.com/CiscoVIRL/schema/v0.95/virl.xsd">
    <extensions>
        <entry key="AutoNetkit.infrastructure_only" type="Boolean">false</entry>
        <entry key="management_network" type="String">flat</entry>
        <entry key="AutoNetkit.enable_cdp" type="Boolean">true</entry>
        <entry key="AutoNetkit.IGP" type="String">ospf</entry>
    </extensions>
    <node name="iosvl2-1" type="SIMPLE" subtype="IOSvL2" location="296,180">
        <extensions>
            <entry key="config" type="string">! IOSvL2 Config generated on 2017-08-27 23:10
! by autonetkit_0.23.5
!
version 15.2
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
service compress-config
no service config
enable password cisco
ip classless
ip subnet-zero
no ip domain lookup
!
line vty 0 4
transport input ssh telnet
exec-timeout 720 0
password cisco
login
!
line con 0
password cisco
!
hostname iosvl2-1
!
boot-start-marker
boot-end-marker
!
!
!
no aaa new-model
!
vtp domain virl.lab
vtp mode transparent
!
vlan 2
  name ank_vlan2
vlan 3
  name ank_vlan3
!
!
!
!
cdp run
!
!
!
ip cef
no ipv6 cef
!
!
spanning-tree mode pvst
spanning-tree extend system-id
!
vlan internal allocation policy ascending
!
!
!
!
vrf definition Mgmt-intf
!
 address-family ipv4
 exit-address-family
 !
 address-family ipv6
 exit-address-family
!
!
!
!
!
interface Loopback0
  description Loopback
!
interface GigabitEthernet0/0
  description OOB management
  ! Configured on launch
  no switchport
  vrf forwarding Mgmt-intf
  no ip address
  no shutdown
!
interface GigabitEthernet0/1
  description to iosvl2-2
  switchport trunk encapsulation dot1q
  switchport mode trunk
  no shutdown
!
interface GigabitEthernet0/2
  description to iosv-1
  switchport access vlan 2
  switchport mode access
  no shutdown
!
interface GigabitEthernet0/3
  description to kali-1
  switchport access vlan 2
  switchport mode access
  no shutdown
!
interface GigabitEthernet1/0
  description to iosv-2
  switchport access vlan 2
  switchport mode access
  no shutdown
!
!
ip forward-protocol nd
!
no ip http server
no ip http secure-server
!
!
!
!
!
!
control-plane
!
!
!
end
        </entry>
            <entry key="AutoNetkit.mgmt_ip" type="string"></entry>
        </extensions>
        <interface id="0" name="GigabitEthernet0/1"/>
        <interface id="1" name="GigabitEthernet0/2"/>
        <interface id="2" name="GigabitEthernet0/3"/>
        <interface id="3" name="GigabitEthernet1/0"/>
        <interface id="4" name="GigabitEthernet1/1"/>
    </node>
    <node name="iosvl2-2" type="SIMPLE" subtype="IOSvL2" location="520,177">
        <extensions>
            <entry key="config" type="string">! IOSvL2 Config generated on 2017-08-27 23:10
! by autonetkit_0.23.5
!
version 15.2
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
service compress-config
no service config
enable password cisco
ip classless
ip subnet-zero
no ip domain lookup
!
line vty 0 4
transport input ssh telnet
exec-timeout 720 0
password cisco
login
!
line con 0
password cisco
!
hostname iosvl2-2
!
boot-start-marker
boot-end-marker
!
!
!
no aaa new-model
!
vtp domain virl.lab
vtp mode transparent
!
vlan 2
  name ank_vlan2
vlan 3
  name ank_vlan3
!
!
!
!
cdp run
!
!
!
ip cef
no ipv6 cef
!
!
spanning-tree mode pvst
spanning-tree extend system-id
!
vlan internal allocation policy ascending
!
!
!
!
vrf definition Mgmt-intf
!
 address-family ipv4
 exit-address-family
 !
 address-family ipv6
 exit-address-family
!
!
!
!
!
interface Loopback0
  description Loopback
!
interface GigabitEthernet0/0
  description OOB management
  ! Configured on launch
  no switchport
  vrf forwarding Mgmt-intf
  no ip address
  no shutdown
!
interface GigabitEthernet0/1
  description to iosvl2-1
  switchport trunk encapsulation dot1q
  switchport mode trunk
  no shutdown
!
interface GigabitEthernet0/2
  description to iosv-1
  switchport access vlan 3
  switchport mode access
  no shutdown
!
interface GigabitEthernet0/3
  description to server-1
  switchport access vlan 3
  switchport mode access
  no shutdown
!
!
ip forward-protocol nd
!
no ip http server
no ip http secure-server
!
!
!
!
!
!
control-plane
!
!
!
end
        </entry>
            <entry key="AutoNetkit.mgmt_ip" type="string"></entry>
        </extensions>
        <interface id="0" name="GigabitEthernet0/1"/>
        <interface id="1" name="GigabitEthernet0/2"/>
        <interface id="2" name="GigabitEthernet0/3"/>
    </node>
    <node name="kali-1" type="SIMPLE" subtype="kali" location="193,282">
        <extensions>
            <entry key="config" type="String">#cloud-config
bootcmd:
- ln -s -t /etc/rc.d /etc/rc.local
hostname: kali-1
manage_etc_hosts: true
package_update: true
packages:
- quagga
bootcmd:
- ip route del default via 172.16.1.1
- ip route add default via 172.16.1.2
runcmd:
- start ttyS0
- systemctl start getty@ttyS0.service
- systemctl start rc-local
- sed -i '/^\s*PasswordAuthentication\s\+no/d' /etc/ssh/sshd_config
- echo "UseDNS no" &gt;&gt; /etc/ssh/sshd_config
- service ssh restart
- systemctl enable zebra ospfd
users:
- default
- gecos: User configured by VIRL Configuration Engine 0.23.10
  lock-passwd: false
  name: cisco
  plain-text-passwd: cisco
  shell: /bin/bash
  ssh-authorized-keys:
  - VIRL-USER-SSH-PUBLIC-KEY
  sudo: ALL=(ALL) ALL
write_files:
- path: /etc/init/ttyS0.conf
  owner: root:root
  content: |
    # ttyS0 - getty
    # This service maintains a getty on ttyS0 from the point the system is
    # started until it is shut down again.
    start on stopped rc or RUNLEVEL=[12345]
    stop on runlevel [!12345]
    respawn
    exec /sbin/getty -L 115200 ttyS0 vt102
  permissions: '0644'
- path: /etc/systemd/system/dhclient@.service
  content: |
    [Unit]
    Description=Run dhclient on %i interface
    After=network.target
    [Service]
    Type=oneshot
    ExecStart=/sbin/dhclient %i -pf /var/run/dhclient.%i.pid -lf /var/lib/dhclient/dhclient.%i.lease
    RemainAfterExit=yes
  owner: root:root
  permissions: '0644'
- path: /etc/network/interfaces
  owner: root:root
  permissions: '0644'
  content: |-
    source-directory /etc/network/interfaces.d
    auto eth0
    iface eth0 inet dhcp
      gateway 172.16.1.2
- path: /etc/rc.local
  owner: root:root
  permissions: '0755'
  content: |-
    #!/bin/sh
    ip route del default
    ip route add default via 172.16.1.2
    ip link set eth1 up
    ip addr add 10.0.0.1/17 dev eth1
    # Use routes from Quagga instead
    #route add -host 192.168.0.1 gw 10.0.0.2 dev eth1
    #route add -host 192.168.0.4 gw 10.0.0.2 dev eth1
    #route add -net 10.0.0.0/17 gw 10.0.0.2 dev eth1
    #route add -net 10.0.128.0/30 gw 10.0.0.2 dev eth1
    #route add -host 192.168.0.1 gw 10.0.0.3 dev eth1
    #route add -host 192.168.0.4 gw 10.0.0.3 dev eth1
    #route add -net 10.0.0.0/17 gw 10.0.0.3 dev eth1
    #route add -net 10.0.128.0/30 gw 10.0.0.3 dev eth1
    exit 0
- path: /etc/network/interfaces.d/eth1
  owner: root:root
  permissions: '0644'
  content: |-
    iface eth1 inet manual
- path: /etc/quagga/zebra.conf
  owner: root:root
  permissions: '0644'
  content: |-
    hostname kali-1
    password cisco
    enable password cisco
    interface eth0
    interface eth1
    line vty
- path: /etc/quagga/ospfd.conf
  owner: root:root
  permissions: '0644'
  content: |-
    hostname kali-1
    password cisco
    log stdout
    interface eth1
      ip ospf cost 1
    router ospf
      ospf router-id 10.0.0.1
      network 10.0.0.1/17 area 0.0.0.0
      network 192.168.0.4/32 area 0.0.0.0
      network 10.0.128.2/32 area 0
    line vty
- path: /root/get-cisco-config.py
  owner: root:root
  permissions: '0755'
  content: |-
    #!/usr/bin/env python
    
    # See
    # http://www.cisco.com/c/en/us/support/docs/ip/simple-network-management-protocol-snmp/15217-copy-configs-snmp.html
    # and
    # http://tools.cisco.com/Support/SNMP/do/BrowseMIB.do?local=en&amp;mibName=CISCO-CONFIG-COPY-MIB
    # for details
    
    from optparse import OptionParser
    from scapy.all import conf,IP,SNMP,SNMPset,ASN1_OID,ASN1_IPADDRESS,UDP,SNMPvarbind,send
    
    parser = OptionParser()
    parser.add_option("-i", "--iface", dest="iface", help="Interface",
                      default="eth1")
    parser.add_option("-s", "--src", dest="srcip", help="Source IP Address",
                      default="192.168.1.2")
    parser.add_option("-d", "--dst", dest="dstip", help="Destination IP Address",
                      default="192.168.1.1")
    parser.add_option("-t", "--tftp", dest="tftpip", help="TFTP Server IP Address",
                      default="192.168.1.2")
    parser.add_option("-f", "--cfg", dest="cfg_file", help="Configuration Filename")
    parser.add_option("-c", "--community", dest="snmpstring",
                      help="SNMP Community Set String", default="secret")
    
    (options, args) = parser.parse_args()
    
    if options.cfg_file is None:
        options.cfg_file = "%s-config" % (options.dstip)
    
    print "Attempting to download IOS config from %s" % (options.dstip)
    
    conf.iface = options.iface
    
    i=IP(src=options.srcip,dst=options.dstip)/UDP(sport=161,dport=161)
    s1=SNMP(
            community=options.snmpstring,
            PDU=SNMPset(
                # iso(1) identified-organization(3) dod(6) internet(1) private(4)
                # enterprise(1) cisco (9) ciscoMgmt(9) ciscoConfigCopyMIB(96)
                # ciscoConfigCopyMIBObjects(1) ccCopy(1) ccCopyTable(1) ccCopyEntry(1)
                # ccCopyEntryRowStatus(14) RANDOM(112)
                varbindlist=[SNMPvarbind(oid=ASN1_OID("1.3.6.1.4.1.9.9.96.1.1.1.1.14.112"),value=6)]
            )
        )
    
    s2=SNMP(
            community=options.snmpstring,
            PDU=SNMPset(
                # iso(1) identified-organization(3) dod(6) internet(1) private(4)
                # enterprise(1) cisco (9) ciscoMgmt(9) ciscoConfigCopyMIB(96)
                # ciscoConfigCopyMIBObjects(1) ccCopy(1) ccCopyTable(1) ccCopyEntry(1)
                # ccCopyProtocol(2) RANDOM(112)
                varbindlist=[SNMPvarbind(oid=ASN1_OID("1.3.6.1.4.1.9.9.96.1.1.1.1.2.112"),value=1)]
            )
        )
    
    s3=SNMP(
            community=options.snmpstring,
            PDU=SNMPset(
                # iso(1) identified-organization(3) dod(6) internet(1) private(4)
                # enterprise(1) cisco (9) ciscoMgmt(9) ciscoConfigCopyMIB(96)
                # ciscoConfigCopyMIBObjects(1) ccCopy(1) ccCopyTable(1) ccCopyEntry(1)
                # ccCopySourceFileType(3) RANDOM(112)
                varbindlist=[SNMPvarbind(oid=ASN1_OID("1.3.6.1.4.1.9.9.96.1.1.1.1.3.112"),value=4)]
            )
        )
    
    s4=SNMP(
            community=options.snmpstring,
            PDU=SNMPset(
                # iso(1) identified-organization(3) dod(6) internet(1) private(4)
                # enterprise(1) cisco (9) ciscoMgmt(9) ciscoConfigCopyMIB(96)
                # ciscoConfigCopyMIBObjects(1) ccCopy(1) ccCopyTable(1) ccCopyEntry(1)
                # ccCopyDestFileType(4) RANDOM(112)
                varbindlist=[SNMPvarbind(oid=ASN1_OID("1.3.6.1.4.1.9.9.96.1.1.1.1.4.112"),value=1)]
            )
        )
    
    s5=SNMP(
            community=options.snmpstring,
            PDU=SNMPset(
                # iso(1) identified-organization(3) dod(6) internet(1) private(4)
                # enterprise(1) cisco (9) ciscoMgmt(9) ciscoConfigCopyMIB(96)
                # ciscoConfigCopyMIBObjects(1) ccCopy(1) ccCopyTable(1) ccCopyEntry(1)
                # ccCopyServerAddress(5) RANDOM(112)
                varbindlist=[SNMPvarbind(oid=ASN1_OID("1.3.6.1.4.1.9.9.96.1.1.1.1.5.112"),value=ASN1_IPADDRESS(options.tftpip))]
            )
        )
    
    s6=SNMP(
            community=options.snmpstring,
            PDU=SNMPset(
                # iso(1) identified-organization(3) dod(6) internet(1) private(4)
                # enterprise(1) cisco (9) ciscoMgmt(9) ciscoConfigCopyMIB(96)
                # ciscoConfigCopyMIBObjects(1) ccCopy(1) ccCopyTable(1) ccCopyEntry(1)
                # ccCopyFileName(6) RANDOM(112)
                varbindlist=[SNMPvarbind(oid=ASN1_OID("1.3.6.1.4.1.9.9.96.1.1.1.1.6.112"),value=options.cfg_file)]
            )
        )
    
    s7=SNMP(
            community=options.snmpstring,
            PDU=SNMPset(
                # iso(1) identified-organization(3) dod(6) internet(1) private(4)
                # enterprise(1) cisco (9) ciscoMgmt(9) ciscoConfigCopyMIB(96)
                # ciscoConfigCopyMIBObjects(1) ccCopy(1) ccCopyTable(1) ccCopyEntry(1)
                # ccCopyEntryRowStatus(14) RANDOM(112)
                varbindlist=[SNMPvarbind(oid=ASN1_OID("1.3.6.1.4.1.9.9.96.1.1.1.1.14.112"),value=1)]
            )
        )
    
    send(i/s1)
    send(i/s2)
    send(i/s3)
    send(i/s4)
    send(i/s5)
    send(i/s6)
    send(i/s7)
- path: /root/merge-cisco-config.py
  owner: root:root
  permissions: '0755'
  content: |-
    #!/usr/bin/env python
    
    # See
    # http://www.cisco.com/c/en/us/support/docs/ip/simple-network-management-protocol-snmp/15217-copy-configs-snmp.html
    # and
    # http://tools.cisco.com/Support/SNMP/do/BrowseMIB.do?local=en&amp;mibName=CISCO-CONFIG-COPY-MIB
    # for details
    
    from optparse import OptionParser
    from scapy.all import conf,IP,SNMP,SNMPset,ASN1_OID,ASN1_IPADDRESS,UDP,SNMPvarbind,send
    
    parser = OptionParser()
    parser.add_option("-i", "--iface", dest="iface", help="Interface",
                      default="eth1")
    parser.add_option("-s", "--src", dest="srcip", help="Source IP Address",
                      default="192.168.1.2")
    parser.add_option("-d", "--dst", dest="dstip", help="Destination IP Address",
                      default="192.168.1.1")
    parser.add_option("-t", "--tftp", dest="tftpip", help="TFTP Server IP Address",
                      default="192.168.1.2")
    parser.add_option("-f", "--cfg", dest="cfg_file", help="Configuration Filename")
    parser.add_option("-c", "--community", dest="snmpstring",
                      help="SNMP Community Set String", default="secret")
    
    (options, args) = parser.parse_args()
    
    if options.cfg_file is None:
        options.cfg_file = "%s-config" % (options.dstip)
    
    print "Attempting to upload IOS config to %s" % (options.dstip)
    
    conf.iface = options.iface
    
    i=IP(src=options.srcip,dst=options.dstip)/UDP(sport=161,dport=161)
    s1=SNMP(
            community=options.snmpstring,
            PDU=SNMPset(
                # iso(1) identified-organization(3) dod(6) internet(1) private(4)
                # enterprise(1) cisco (9) ciscoMgmt(9) ciscoConfigCopyMIB(96)
                # ciscoConfigCopyMIBObjects(1) ccCopy(1) ccCopyTable(1) ccCopyEntry(1)
                # ccCopyEntryRowStatus(14) RANDOM(112)
                varbindlist=[SNMPvarbind(oid=ASN1_OID("1.3.6.1.4.1.9.9.96.1.1.1.1.14.112"),value=6)]
            )
        )
    
    s2=SNMP(
            community=options.snmpstring,
            PDU=SNMPset(
                # iso(1) identified-organization(3) dod(6) internet(1) private(4)
                # enterprise(1) cisco (9) ciscoMgmt(9) ciscoConfigCopyMIB(96)
                # ciscoConfigCopyMIBObjects(1) ccCopy(1) ccCopyTable(1) ccCopyEntry(1)
                # ccCopyProtocol(2) RANDOM(112)
                varbindlist=[SNMPvarbind(oid=ASN1_OID("1.3.6.1.4.1.9.9.96.1.1.1.1.2.112"),value=1)]
            )
        )
    
    s3=SNMP(
            community=options.snmpstring,
            PDU=SNMPset(
                # iso(1) identified-organization(3) dod(6) internet(1) private(4)
                # enterprise(1) cisco (9) ciscoMgmt(9) ciscoConfigCopyMIB(96)
                # ciscoConfigCopyMIBObjects(1) ccCopy(1) ccCopyTable(1) ccCopyEntry(1)
                # ccCopySourceFileType(3) RANDOM(112)
                varbindlist=[SNMPvarbind(oid=ASN1_OID("1.3.6.1.4.1.9.9.96.1.1.1.1.3.112"),value=1)]
            )
        )
    
    s4=SNMP(
            community=options.snmpstring,
            PDU=SNMPset(
                # iso(1) identified-organization(3) dod(6) internet(1) private(4)
                # enterprise(1) cisco (9) ciscoMgmt(9) ciscoConfigCopyMIB(96)
                # ciscoConfigCopyMIBObjects(1) ccCopy(1) ccCopyTable(1) ccCopyEntry(1)
                # ccCopyDestFileType(4) RANDOM(112)
                varbindlist=[SNMPvarbind(oid=ASN1_OID("1.3.6.1.4.1.9.9.96.1.1.1.1.4.112"),value=4)]
            )
        )
    
    s5=SNMP(
            community=options.snmpstring,
            PDU=SNMPset(
                # iso(1) identified-organization(3) dod(6) internet(1) private(4)
                # enterprise(1) cisco (9) ciscoMgmt(9) ciscoConfigCopyMIB(96)
                # ciscoConfigCopyMIBObjects(1) ccCopy(1) ccCopyTable(1) ccCopyEntry(1)
                # ccCopyServerAddress(5) RANDOM(112)
                varbindlist=[SNMPvarbind(oid=ASN1_OID("1.3.6.1.4.1.9.9.96.1.1.1.1.5.112"),value=ASN1_IPADDRESS(options.tftpip))]
            )
        )
    
    s6=SNMP(
            community=options.snmpstring,
            PDU=SNMPset(
                # iso(1) identified-organization(3) dod(6) internet(1) private(4)
                # enterprise(1) cisco (9) ciscoMgmt(9) ciscoConfigCopyMIB(96)
                # ciscoConfigCopyMIBObjects(1) ccCopy(1) ccCopyTable(1) ccCopyEntry(1)
                # ccCopyFileName(6) RANDOM(112)
                varbindlist=[SNMPvarbind(oid=ASN1_OID("1.3.6.1.4.1.9.9.96.1.1.1.1.6.112"),value=options.cfg_file)]
            )
        )
    
    s7=SNMP(
            community=options.snmpstring,
            PDU=SNMPset(
                # iso(1) identified-organization(3) dod(6) internet(1) private(4)
                # enterprise(1) cisco (9) ciscoMgmt(9) ciscoConfigCopyMIB(96)
                # ciscoConfigCopyMIBObjects(1) ccCopy(1) ccCopyTable(1) ccCopyEntry(1)
                # ccCopyEntryRowStatus(14) RANDOM(112)
                varbindlist=[SNMPvarbind(oid=ASN1_OID("1.3.6.1.4.1.9.9.96.1.1.1.1.14.112"),value=1)]
            )
        )
    
    send(i/s1)
    send(i/s2)
    send(i/s3)
    send(i/s4)
    send(i/s5)
    send(i/s6)
    send(i/s7)
- path: /etc/default/atftpd
  owner: root:root
  permissions: '0644'
  content: |-
    USE_INETD=false
    # OPTIONS below are used only with init script
    OPTIONS="--tftpd-timeout 300 --retry-timeout 5 --mcast-port 1758 --mcast-addr 239.239.239.0-255 --mcast-ttl 1 --maxthread 100 --verbose=5 /srv/tftp"
- path: /srv/tftp/router.cfg
  owner: nobody:nogroup
  permissions: '0644'
  content: |-
    !
    ! Last configuration change at 23:19:07 UTC Tue Aug 29 2017 by cisco
    !
    version 15.6
    service timestamps debug datetime msec
    service timestamps log datetime msec
    service password-encryption
    !
    hostname iosv-2
    !
    boot-start-marker
    boot-end-marker
    !
    !
    vrf definition Mgmt-intf
     !
     address-family ipv4
     exit-address-family
     !
     address-family ipv6
     exit-address-family
    !
    enable password 7 060506324F41
    !
    aaa new-model
    !
    !
    aaa authentication login default group radius local line
    aaa authorization exec default group radius if-authenticated 
    !
    !
    !
    !
    !
    aaa session-id common
    ethernet lmi ce
    !
    !
    !
    mmi polling-interval 60
    no mmi auto-configure
    no mmi pvc
    mmi snmp-timeout 180
    !
    !
    !
    !
    !
    !
    !
    !
    !
    !
    !
    no ip domain lookup
    ip domain name virl.info
    ip cef
    ipv6 unicast-routing
    ipv6 cef
    !
    multilink bundle-name authenticated
    !
    !
    !
    !
    username cisco privilege 15 secret 5 $1$WaUX$blEhl/Fee6CSV8WMIvhv4.
    !
    redundancy
    !
    !
    ! 
    !
    !
    !
    !
    !
    !
    !
    !
    !
    !
    !
    !
    interface Loopback0
     description Loopback
     ip address 192.168.0.4 255.255.255.255
    !
    interface GigabitEthernet0/0
     description OOB Management
     vrf forwarding Mgmt-intf
     ip address 172.16.1.191 255.255.255.0
     duplex full
     speed auto
     media-type rj45
    !
    interface GigabitEthernet0/1
     description to iosvl2-1
     ip address 10.0.0.3 255.255.128.0
     ip ospf cost 1
     duplex full
     speed auto
     media-type rj45
    !
    router ospf 1
     passive-interface Loopback0
     network 10.0.0.0 0.0.127.255 area 0
     network 192.168.0.4 0.0.0.0 area 0
    !
    router bgp 1
     bgp router-id 192.168.0.4
     bgp log-neighbor-changes
     neighbor 192.168.0.1 remote-as 1
     neighbor 192.168.0.1 description iBGP peer iosv-1
     neighbor 192.168.0.1 update-source Loopback0
     !
     address-family ipv4
      network 192.168.0.4 mask 255.255.255.255
      neighbor 192.168.0.1 activate
     exit-address-family
    !
    ip forward-protocol nd
    !
    !
    no ip http server
    no ip http secure-server
    ip ssh server algorithm authentication password
    !
    ip access-list standard IN-VTY
     permit 172.16.1.0 0.0.0.255
     permit 192.168.0.0 0.0.0.255
     permit 10.0.128.0 0.0.0.255
    ip access-list standard SNMP-RW
     permit 172.16.1.0 0.0.0.255
     permit 192.168.0.0 0.0.0.255
     permit 10.0.128.0 0.0.0.3
    !
    ip radius source-interface Loopback0 
    !
    snmp-server community supersecret RW SNMP-RW
    snmp-server chassis-id 
    !
    !
    !
    radius server RADIUS
     address ipv4 10.0.128.2 auth-port 1812 acct-port 1813
     key 7 13061E0108030723382727
    !
    !
    control-plane
    !
    banner exec ^
    **************************************************************************
    * IOSv - Cisco Systems Confidential                                      *
    *                                                                        *
    * Supplemental End User License Restrictions                             *
    *                                                                        *
    * This IOSv software is provided AS-IS without warranty of any kind.     *
    * Under no circumstances may this software be used separate from         *
    * the Cisco Modeling Labs Software that this software was provided       *
    *  with, or deployed or used as part of a production environment.        *
    *                                                                        *
    * By using the software, you agree to abide by the terms and             *
    * conditions of the Cisco End User License Agreement at                  *
    * http://www.cisco.com/go/eula.                                          *
    *                                                                        *
    * Unauthorized use or distribution of this software is expressly         *
    * prohibited.                                                            *
    **************************************************************************
    ^
    banner incoming ^
    **************************************************************************
    * IOSv - Cisco Systems Confidential                                      *
    *                                                                        *
    * Supplemental End User License Restrictions                             *
    *                                                                        *
    * This IOSv software is provided AS-IS without warranty of any kind.     *
    * Under no circumstances may this software be used separate from         *
    * the Cisco Modeling Labs Software that this software was provided       *
    *  with, or deployed or used as part of a production environment.        *
    *                                                                        *
    * By using the software, you agree to abide by the terms and             *
    * conditions of the Cisco End User License Agreement at                  *
    * http://www.cisco.com/go/eula.                                          *
    *                                                                        *
    * Unauthorized use or distribution of this software is expressly         *
    * prohibited.                                                            *
    **************************************************************************
    ^
    banner login ^
    **************************************************************************
    * IOSv - Cisco Systems Confidential                                      *
    *                                                                        *
    * Supplemental End User License Restrictions                             *
    *                                                                        *
    * This IOSv software is provided AS-IS without warranty of any kind.     *
    * Under no circumstances may this software be used separate from         *
    * the Cisco Modeling Labs Software that this software was provided       *
    *  with, or deployed or used as part of a production environment.        *
    *                                                                        *
    * By using the software, you agree to abide by the terms and             *
    * conditions of the Cisco End User License Agreement at                  *
    * http://www.cisco.com/go/eula.                                          *
    *                                                                        *
    * Unauthorized use or distribution of this software is expressly         *
    * prohibited.                                                            *
    **************************************************************************
    ^
    !
    line con 0
     password 7 0822455D0A16
    line aux 0
    line vty 0 4
     exec-timeout 720 0
     password 7 1511021F0725
     transport input telnet ssh
    !
    no scheduler allocate
    !
    end
</entry>
        </extensions>
        <interface id="0" name="eth1" ipv4="10.0.0.1" netPrefixLenV4="17">
            <extensions>
                <entry key="AutoNetkit.vlan" type="Integer">2</entry>
            </extensions>
        </interface>
    </node>
    <node name="iosv-1" type="SIMPLE" subtype="IOSv" location="417,76" ipv4="192.168.0.1">
        <extensions>
            <entry key="AutoNetkit.mgmt_ip" type="string"></entry>
            <entry key="config" type="String">! IOS Config generated on 2017-08-27 23:10
! by autonetkit_0.23.5
!
hostname iosv-1
boot-start-marker
boot-end-marker
!
vrf definition Mgmt-intf
!
 address-family ipv4
 exit-address-family
 !
 address-family ipv6
 exit-address-family
!
!
!
no aaa new-model
!
!
ip cef
ipv6 unicast-routing
ipv6 cef
!
!
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
no service config
enable password cisco
ip classless
ip subnet-zero
no ip domain lookup
ip domain name virl.info
crypto key generate rsa modulus 768
ip ssh server algorithm authentication password
username cisco privilege 15 secret cisco
ip access-list standard IN-VTY
  permit 172.16.1.0 0.0.0.255
  permit 192.168.0.0 0.0.0.255
  permit 10.0.128.0 0.0.0.255
ip access-list standard SNMP-RW
  permit 172.16.1.0 0.0.0.255
  permit 192.168.0.0 0.0.0.255
  permit 10.0.128.0 0.0.0.3
snmp-server community supersecret rw SNMP-RW
line vty 0 4
   transport input ssh telnet
   access-class IN-VTY in vrf-also
   exec-timeout 720 0
   password cisco
   login local
 line con 0
   password cisco
!
cdp run
!
!
interface Loopback0
  description Loopback
  ip address 192.168.0.1 255.255.255.255
!
interface GigabitEthernet0/0
  description OOB Management
  vrf forwarding Mgmt-intf
  ! Configured on launch
  no ip address
  cdp enable
  duplex full
  speed auto
  no shutdown
!
interface GigabitEthernet0/1
  description to iosvl2-1
  ip address 10.0.0.2 255.255.128.0
  cdp enable
  ip ospf cost 1
  duplex full
  speed auto
  no shutdown
!
interface GigabitEthernet0/2
  description to iosvl2-2
  ip address 10.0.128.1 255.255.255.252
  cdp enable
  ip ospf cost 1
  duplex full
  speed auto
  no shutdown
!
interface GigabitEthernet0/3
  description to admin-1
  ip address 10.0.128.5 255.255.255.252
  cdp enable
  ip ospf cost 1
  duplex full
  speed auto
  no shutdown
!
!
!
router ospf 1
  network 192.168.0.1 0.0.0.0 area 0
  log-adjacency-changes
  passive-interface Loopback0
  network 10.0.0.0 0.0.127.255 area 0
  network 10.0.128.0 0.0.0.3 area 0
  network 10.0.128.4 0.0.0.3 area 0
!
!
router bgp 1
  bgp router-id 192.168.0.1
  no synchronization
! ibgp
  ! ibgp peers
  !
  neighbor 192.168.0.4 remote-as 1
  neighbor 192.168.0.4 description iBGP peer iosv-2
  neighbor 192.168.0.4 update-source Loopback0
!
!
 !
 address-family ipv4
  network 192.168.0.1 mask 255.255.255.255
  neighbor 192.168.0.4 activate
 exit-address-family
!
!
!
end</entry>
        </extensions>
        <interface id="0" name="GigabitEthernet0/1" ipv4="10.0.0.2" netPrefixLenV4="17">
            <extensions>
                <entry key="AutoNetkit.vlan" type="Integer">2</entry>
            </extensions>
        </interface>
        <interface id="1" name="GigabitEthernet0/2" ipv4="10.0.128.1" netPrefixLenV4="30">
            <extensions>
                <entry key="AutoNetkit.vlan" type="Integer">3</entry>
            </extensions>
        </interface>
        <interface id="2" name="GigabitEthernet0/3"/>
    </node>
    <node name="server-1" type="SIMPLE" subtype="server" location="592,287">
        <extensions>
            <entry key="config" type="String">#cloud-config
bootcmd:
- ln -s -t /etc/rc.d /etc/rc.local
hostname: server-1
manage_etc_hosts: true
package_update: true
packages:
- snmp
- freeradius
- tshark
runcmd:
- start ttyS0
- systemctl start getty@ttyS0.service
- systemctl start rc-local
- sed -i '/^\s*PasswordAuthentication\s\+no/d' /etc/ssh/sshd_config
- echo "UseDNS no" &gt;&gt; /etc/ssh/sshd_config
- service ssh restart
- service sshd restart
- cp /tmp/clients.conf.new /etc/freeradius/clients.conf
- cp /tmp/users.new /etc/freeradius/users
- systemctl enable freeradius
- systemctl start freeradius
- chown -R cisco:cisco /home/cisco
- sudo -u cisco /home/cisco/http-chatter.sh &amp;
- sudo -u cisco /home/cisco/snmp-chatter.sh &amp;
users:
- default
- gecos: User configured by VIRL Configuration Engine 0.23.10
  lock-passwd: false
  name: cisco
  plain-text-passwd: cisco
  shell: /bin/bash
  ssh-authorized-keys:
  - VIRL-USER-SSH-PUBLIC-KEY
  sudo: ALL=(ALL) ALL
write_files:
- path: /etc/init/ttyS0.conf
  owner: root:root
  content: |
    # ttyS0 - getty
    # This service maintains a getty on ttyS0 from the point the system is
    # started until it is shut down again.
    start on stopped rc or RUNLEVEL=[12345]
    stop on runlevel [!12345]
    respawn
    exec /sbin/getty -L 115200 ttyS0 vt102
  permissions: '0644'
- path: /etc/systemd/system/dhclient@.service
  content: |
    [Unit]
    Description=Run dhclient on %i interface
    After=network.target
    [Service]
    Type=oneshot
    ExecStart=/sbin/dhclient %i -pf /var/run/dhclient.%i.pid -lf /var/lib/dhclient/dhclient.%i.lease
    RemainAfterExit=yes
  owner: root:root
  permissions: '0644'
- path: /etc/rc.local
  owner: root:root
  permissions: '0755'
  content: |-
    #!/bin/sh
    ip route del default
    ip route add default via 172.16.1.2
    ifconfig eth1 up 10.0.128.2 netmask 255.255.255.252
    route add -host 192.168.0.1 gw 10.0.128.1 dev eth1
    route add -host 192.168.0.4 gw 10.0.128.1 dev eth1
    route add -net 10.0.0.0/17 gw 10.0.128.1 dev eth1
    route add -net 10.0.128.0/30 gw 10.0.128.1 dev eth1
    exit 0
- path: /tmp/clients.conf.new
  content: |
    client 192.168.0.0/24 {
    secret = ciscocisco
    nastype = cisco
    shortname = virl
    }
  owner: "root:root"
  permissions: '0640'
- path: /tmp/users.new
  content: |
    admin Cleartext-Password := "secret123"
      Service-Type = NAS-Prompt-User,
      Cisco-AVPair = "shell:priv-lvl=15"
  owner: "root:root"
  permissions: '0640'
- path: /home/cisco/http-chatter.sh
  content: |
    #!/bin/bash
    while true; do
      curl -u admin:secret123 http://192.168.0.4
      sleep 15
    done
  owner: "root:root"
  permissions: '0755'
- path: /home/cisco/snmp-chatter.sh
  content: |
    #!/bin/bash
    while true; do
      snmpget -v 2c -c supersecret 192.168.0.4 1.3.6.1.2.1.1.1.0
      sleep 15
    done
  owner: "root:root"
  permissions: '0755'

</entry>
        </extensions>
        <interface id="0" name="eth1" ipv4="10.0.128.2" netPrefixLenV4="30">
            <extensions>
                <entry key="AutoNetkit.vlan" type="Integer">3</entry>
            </extensions>
        </interface>
    </node>
    <node name="iosv-2" type="SIMPLE" subtype="IOSv" location="370,291" ipv4="192.168.0.4">
        <extensions>
            <entry key="AutoNetkit.mgmt_ip" type="string"></entry>
            <entry key="config" type="String">! IOS Config generated on 2017-08-27 23:10
! by autonetkit_0.23.5
!
version 15.6
service timestamps debug datetime msec
service timestamps log datetime msec
service password-encryption
!
hostname iosv-2
!
boot-start-marker
boot-end-marker
!
!
vrf definition Mgmt-intf
 !
 address-family ipv4
 exit-address-family
 !
 address-family ipv6
 exit-address-family
!
enable password 7 060506324F41
!
aaa new-model
!
!
aaa authentication login default group radius local line
aaa authorization exec default group radius if-authenticated
!
!
!
!
!
aaa session-id common
ethernet lmi ce
!
!
!
mmi polling-interval 60
no mmi auto-configure
no mmi pvc
mmi snmp-timeout 180
!
!
!
!
!
!
!
!
!
!
!
no ip domain lookup
ip domain name virl.info
ip cef
ipv6 unicast-routing
ipv6 cef
!
multilink bundle-name authenticated
!
!
!
!
username cisco privilege 15 secret 5 $1$WaUX$blEhl/Fee6CSV8WMIvhv4.
!
redundancy
!
!
! 
!
!
!
!
!
!
!
!
!
!
!
!
interface Loopback0
 description Loopback
 ip address 192.168.0.4 255.255.255.255
!
interface GigabitEthernet0/0
 description OOB Management
 vrf forwarding Mgmt-intf
 ip address 172.16.1.182 255.255.255.0
 duplex full
 speed auto
 media-type rj45
!
interface GigabitEthernet0/1
 description to iosvl2-1
 ip address 10.0.0.3 255.255.128.0
 ip ospf cost 1
 duplex full
 speed auto
 media-type rj45
!
router ospf 1
 passive-interface Loopback0
 network 10.0.0.0 0.0.127.255 area 0
 network 192.168.0.4 0.0.0.0 area 0
!
router bgp 1
 bgp router-id 192.168.0.4
 bgp log-neighbor-changes
 neighbor 192.168.0.1 remote-as 1
 neighbor 192.168.0.1 description iBGP peer iosv-1
 neighbor 192.168.0.1 update-source Loopback0
 !
 address-family ipv4
  network 192.168.0.4 mask 255.255.255.255
  neighbor 192.168.0.1 activate
 exit-address-family
!
ip forward-protocol nd
!
!
ip http server
ip http authentication aaa login-authentication default
no ip http secure-server
ip ssh server algorithm authentication password
!
ip access-list standard SNMP-RW
 permit 172.16.1.0 0.0.0.255
 permit 192.168.0.0 0.0.0.255
 permit 10.0.128.0 0.0.0.3
!
ip radius source-interface Loopback0 
!
snmp-server community supersecret RW SNMP-RW
snmp-server chassis-id 
!
!
!
radius server RADIUS
 address ipv4 10.0.128.2 auth-port 1812 acct-port 1813
 key 7 13061E0108030723382727
!
!
control-plane
!
banner exec ^
**************************************************************************
* IOSv - Cisco Systems Confidential                                      *
*                                                                        *
* Supplemental End User License Restrictions                             *
*                                                                        *
* This IOSv software is provided AS-IS without warranty of any kind.     *
* Under no circumstances may this software be used separate from         *
* the Cisco Modeling Labs Software that this software was provided       *
*  with, or deployed or used as part of a production environment.        *
*                                                                        *
* By using the software, you agree to abide by the terms and             *
* conditions of the Cisco End User License Agreement at                  *
* http://www.cisco.com/go/eula.                                          *
*                                                                        *
* Unauthorized use or distribution of this software is expressly         *
* prohibited.                                                            *
**************************************************************************
^
banner incoming ^
**************************************************************************
* IOSv - Cisco Systems Confidential                                      *
*                                                                        *
* Supplemental End User License Restrictions                             *
*                                                                        *
* This IOSv software is provided AS-IS without warranty of any kind.     *
* Under no circumstances may this software be used separate from         *
* the Cisco Modeling Labs Software that this software was provided       *
*  with, or deployed or used as part of a production environment.        *
*                                                                        *
* By using the software, you agree to abide by the terms and             *
* conditions of the Cisco End User License Agreement at                  *
* http://www.cisco.com/go/eula.                                          *
*                                                                        *
* Unauthorized use or distribution of this software is expressly         *
* prohibited.                                                            *
**************************************************************************
^
banner login ^
**************************************************************************
* IOSv - Cisco Systems Confidential                                      *
*                                                                        *
* Supplemental End User License Restrictions                             *
*                                                                        *
* This IOSv software is provided AS-IS without warranty of any kind.     *
* Under no circumstances may this software be used separate from         *
* the Cisco Modeling Labs Software that this software was provided       *
*  with, or deployed or used as part of a production environment.        *
*                                                                        *
* By using the software, you agree to abide by the terms and             *
* conditions of the Cisco End User License Agreement at                  *
* http://www.cisco.com/go/eula.                                          *
*                                                                        *
* Unauthorized use or distribution of this software is expressly         *
* prohibited.                                                            *
**************************************************************************
^
!
line con 0
 password 7 0822455D0A16
line aux 0
line vty 0 4
 exec-timeout 720 0
 password 7 1511021F0725
 transport input telnet ssh
!
no scheduler allocate
!
end</entry>
        </extensions>
        <interface id="0" name="GigabitEthernet0/1" ipv4="10.0.0.3" netPrefixLenV4="17">
            <extensions>
                <entry key="AutoNetkit.vlan" type="Integer">2</entry>
            </extensions>
        </interface>
    </node>
    <node name="admin-1" type="SIMPLE" subtype="lxc" location="605,72">
        <extensions>
            <entry key="config" type="String">#cloud-config
bootcmd:
- ln -s -t /etc/rc.d /etc/rc.local
hostname: admin-1
manage_etc_hosts: true
runcmd:
- systemctl start rc-local
- sed -i '/^\s*PasswordAuthentication\s\+no/d' /etc/ssh/sshd_config
- echo "UseDNS no" &gt;&gt; /etc/ssh/sshd_config
- service ssh restart
- service sshd restart
users:
- default
- gecos: User configured by VIRL Configuration Engine 0.23.10
  lock-passwd: false
  name: cisco
  plain-text-passwd: cisco
  shell: /bin/bash
  ssh-authorized-keys:
  - VIRL-USER-SSH-PUBLIC-KEY
  sudo: ALL=(ALL) ALL
write_files:
- path: /etc/systemd/system/dhclient@.service
  content: |
    [Unit]
    Description=Run dhclient on %i interface
    After=network.target
    [Service]
    Type=oneshot
    ExecStart=/sbin/dhclient %i -pf /var/run/dhclient.%i.pid -lf /var/lib/dhclient/dhclient.%i.lease
    RemainAfterExit=yes
  owner: root:root
  permissions: '0644'
- path: /etc/rc.local
  owner: root:root
  permissions: '0755'
  content: |-
    #!/bin/sh
    ifconfig eth1 up 10.0.128.6 netmask 255.255.255.252
    route add -host 192.168.0.1 gw 10.0.128.5 dev eth1
    route add -host 192.168.0.4 gw 10.0.128.5 dev eth1
    route add -net 10.0.0.0/16 gw 10.0.128.5 dev eth1
    route add -host 192.168.0.1 gw 10.0.128.5 dev eth1
    route add -host 192.168.0.4 gw 10.0.128.5 dev eth1
    exit 0
</entry>
        </extensions>
        <interface id="0" name="eth1"/>
    </node>
    <annotations/>
    <connection dst="/virl:topology/virl:node[2]/virl:interface[1]" src="/virl:topology/virl:node[1]/virl:interface[1]"/>
    <connection dst="/virl:topology/virl:node[1]/virl:interface[2]" src="/virl:topology/virl:node[4]/virl:interface[1]"/>
    <connection dst="/virl:topology/virl:node[4]/virl:interface[2]" src="/virl:topology/virl:node[2]/virl:interface[2]"/>
    <connection dst="/virl:topology/virl:node[1]/virl:interface[3]" src="/virl:topology/virl:node[3]/virl:interface[1]"/>
    <connection dst="/virl:topology/virl:node[2]/virl:interface[3]" src="/virl:topology/virl:node[5]/virl:interface[1]"/>
    <connection dst="/virl:topology/virl:node[6]/virl:interface[1]" src="/virl:topology/virl:node[1]/virl:interface[4]"/>
    <connection dst="/virl:topology/virl:node[7]/virl:interface[1]" src="/virl:topology/virl:node[4]/virl:interface[3]"/>
</topology>
