From 2d16761887d7fb80da131b5cf38e32bcc94a3011 Mon Sep 17 00:00:00 2001
From: Tectas <adrian.stoeckl@gmail.com>
Date: Mon, 17 Nov 2014 21:21:08 +0100
Subject: [PATCH] arch/arm/boot/dts: Raise max microvolt at cpu for pm8941 and
 pma8084

---
 arch/arm/boot/dts/msm8974pro-pm8941.dtsi            | 8 ++++----
 arch/arm/boot/dts/msm8974pro-pma8084-regulator.dtsi | 8 ++++----
 2 files changed, 8 insertions(+), 8 deletions(-)

diff --git a/arch/arm/boot/dts/msm8974pro-pm8941.dtsi b/arch/arm/boot/dts/msm8974pro-pm8941.dtsi
index b5020789bbb..2c5dd3d4416 100644
--- a/arch/arm/boot/dts/msm8974pro-pm8941.dtsi
+++ b/arch/arm/boot/dts/msm8974pro-pm8941.dtsi
@@ -39,22 +39,22 @@
 };
 
 &krait0_vreg {
-		regulator-max-microvolt = <1120000>;
+		regulator-max-microvolt = <1180000>;
 		qcom,ldo-delta-voltage = <12500>;
 };
 
 &krait1_vreg {
-		regulator-max-microvolt = <1120000>;
+		regulator-max-microvolt = <1180000>;
 		qcom,ldo-delta-voltage = <12500>;
 };
 
 &krait2_vreg {
-		regulator-max-microvolt = <1120000>;
+		regulator-max-microvolt = <1180000>;
 		qcom,ldo-delta-voltage = <12500>;
 };
 
 &krait3_vreg {
-		regulator-max-microvolt = <1120000>;
+		regulator-max-microvolt = <1180000>;
 		qcom,ldo-delta-voltage = <12500>;
 };
 
diff --git a/arch/arm/boot/dts/msm8974pro-pma8084-regulator.dtsi b/arch/arm/boot/dts/msm8974pro-pma8084-regulator.dtsi
index 433d466a3ee..8674dee3096 100644
--- a/arch/arm/boot/dts/msm8974pro-pma8084-regulator.dtsi
+++ b/arch/arm/boot/dts/msm8974pro-pma8084-regulator.dtsi
@@ -492,7 +492,7 @@
 				<0xf908a800 0x1000>; /* APCS_ALIAS0_KPSS_MDD */
 			reg-names = "acs", "mdd";
 			regulator-min-microvolt = <500000>;
-			regulator-max-microvolt = <1120000>;
+			regulator-max-microvolt = <1180000>;
 			qcom,headroom-voltage = <150000>;
 			qcom,retention-voltage = <675000>;
 			qcom,ldo-default-voltage = <750000>;
@@ -508,7 +508,7 @@
 				<0xf909a800 0x1000>; /* APCS_ALIAS1_KPSS_MDD */
 			reg-names = "acs", "mdd";
 			regulator-min-microvolt = <500000>;
-			regulator-max-microvolt = <1120000>;
+			regulator-max-microvolt = <1180000>;
 			qcom,headroom-voltage = <150000>;
 			qcom,retention-voltage = <675000>;
 			qcom,ldo-default-voltage = <750000>;
@@ -524,7 +524,7 @@
 				<0xf90aa800 0x1000>; /* APCS_ALIAS2_KPSS_MDD */
 			reg-names = "acs", "mdd";
 			regulator-min-microvolt = <500000>;
-			regulator-max-microvolt = <1120000>;
+			regulator-max-microvolt = <1180000>;
 			qcom,headroom-voltage = <150000>;
 			qcom,retention-voltage = <675000>;
 			qcom,ldo-default-voltage = <750000>;
@@ -540,7 +540,7 @@
 				<0xf90ba800 0x1000>; /* APCS_ALIAS3_KPSS_MDD */
 			reg-names = "acs", "mdd";
 			regulator-min-microvolt = <500000>;
-			regulator-max-microvolt = <1120000>;
+			regulator-max-microvolt = <1180000>;
 			qcom,headroom-voltage = <150000>;
 			qcom,retention-voltage = <675000>;
 			qcom,ldo-default-voltage = <750000>;
