From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Devin Moore <devinmoore@google.com>
Date: Tue, 25 Apr 2023 00:17:13 +0000
Subject: [PATCH] Allow sensors list to be empty

Test: atest VtsHalSensorManagerV1_0TargetTest
Bug: 278013275
Bug: 269014004
(cherry picked from https://googleplex-android-review.googlesource.com/q/commit:49600b10aa5675d4e7e985203d69f252ead13e45)
(cherry picked from https://googleplex-android-review.googlesource.com/q/commit:7057a9f08d98bfec8ffbabcf00f2885d3909c6c9)
Merged-In: I091f57de9570b0ace3a8da76f16fe0e83f0aa624
Change-Id: I091f57de9570b0ace3a8da76f16fe0e83f0aa624
---
 libs/sensor/SensorManager.cpp | 7 ++-----
 1 file changed, 2 insertions(+), 5 deletions(-)

diff --git a/libs/sensor/SensorManager.cpp b/libs/sensor/SensorManager.cpp
index d7210b10e0..35802db95c 100644
--- a/libs/sensor/SensorManager.cpp
+++ b/libs/sensor/SensorManager.cpp
@@ -172,11 +172,8 @@ status_t SensorManager::assertStateLocked() {
 
         mSensors = mSensorServer->getSensorList(mOpPackageName);
         size_t count = mSensors.size();
-        if (count == 0) {
-            ALOGE("Failed to get Sensor list");
-            mSensorServer.clear();
-            return UNKNOWN_ERROR;
-        }
+        // If count is 0, mSensorList will be non-null. This is old
+        // existing behavior and callers expect this.
         mSensorList =
                 static_cast<Sensor const**>(malloc(count * sizeof(Sensor*)));
         LOG_ALWAYS_FATAL_IF(mSensorList == NULL, "mSensorList NULL");
