<?xml version="1.0" encoding="UTF-8"?>
<!-- STM32F0xx board Template -->
<board
  xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance"
  xsi:noNamespaceSchemaLocation="http://www.chibios.org/xml/schema/boards/stm32f0xx_board.xsd">
  <configuration_settings>
    <templates_path>resources/gencfg/processors/boards/stm32f0xx/templates</templates_path>
    <output_path>..</output_path>
  </configuration_settings>
  <board_name>ST STM32F0-Discovery</board_name>
  <board_id>ST_STM32F0_DISCOVERY</board_id>
  <board_functions></board_functions>
  <subtype>STM32F0XX_MD</subtype>
  <clocks HSEFrequency="0" HSEBypass="true" LSEFrequency="0"
  	LSEBypass="false" LSEDrive="3 High Drive (default)" />
  <ports>
    <GPIOA>
      <pin0
        ID="BUTTON"
        Type="PushPull"
        Speed="Minimum"
        Resistor="Floating"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin1
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin2
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin3
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin4
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin5
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin6
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin7
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin8
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin9
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin10
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin11
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin12
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin13
        ID="SWDAT"
        Type="PushPull"
        Speed="Maximum"
        Resistor="PullUp"
        Level="High"
        Mode="Alternate"
        Alternate="0" />
      <pin14
        ID="SWCLK"
        Type="PushPull"
        Speed="Maximum"
        Resistor="PullDown"
        Level="High"
        Mode="Alternate"
        Alternate="0" />
      <pin15
        ID=""
        Type="PushPull"
        Speed="Maximum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
    </GPIOA>
    <GPIOB>
      <pin0
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin1
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin2
        ID=""
        Type="PushPull"
        Speed="Maximum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin3
        ID=""
        Type="PushPull"
        Speed="Maximum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin4
        ID=""
        Type="PushPull"
        Speed="Maximum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin5
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin6
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin7
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin8
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin9
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin10
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin11
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin12
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin13
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin14
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin15
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
    </GPIOB>
    <GPIOC>
      <pin0
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin1
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin2
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin3
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin4
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin5
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin6
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin7
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin8
        ID="LED4"
        Type="PushPull"
        Speed="Maximum"
        Resistor="Floating"
        Level="Low"
        Mode="Output"
        Alternate="0" />
      <pin9
        ID="LED3"
        Type="PushPull"
        Speed="Maximum"
        Resistor="Floating"
        Level="Low"
        Mode="Output"
        Alternate="0" />
      <pin10
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin11
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin12
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin13
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin14
        ID="OSC32_IN"
        Type="PushPull"
        Speed="Maximum"
        Resistor="Floating"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin15
        ID="OSC32_OUT"
        Type="PushPull"
        Speed="Maximum"
        Resistor="Floating"
        Level="High"
        Mode="Input"
        Alternate="0" />
    </GPIOC>
    <GPIOD>
      <pin0
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin1
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin2
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin3
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin4
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin5
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin6
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin7
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin8
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin9
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin10
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin11
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin12
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin13
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin14
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin15
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
    </GPIOD>
    <GPIOF>
      <pin0
        ID="OSC_IN"
        Type="PushPull"
        Speed="Minimum"
        Resistor="Floating"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin1
        ID="OSC_OUT"
        Type="PushPull"
        Speed="Minimum"
        Resistor="Floating"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin2
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin3
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin4
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin5
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin6
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin7
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin8
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin9
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin10
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin11
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin12
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin13
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin14
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
      <pin15
        ID=""
        Type="PushPull"
        Speed="Minimum"
        Resistor="PullUp"
        Level="High"
        Mode="Input"
        Alternate="0" />
    </GPIOF>
  </ports>
</board>
