Cmp-Mod V01 Created by CvPcb (2014-03-01 BZR 4730)-product date = Tuesday, August 26, 2014 'AMt' 09:05:06 AM

BeginCmp
TimeStamp = /53A8C780/53A8D535;
Reference = BT1;
ValeurCmp = BATTERY;
IdModule  = bat_coin:MPD_BU2032SM-BT-G;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53A8C6A5;
Reference = C2;
ValeurCmp = 100N;
IdModule  = ipc_capc:IPC_CAPC1005X55N;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53A8C69F;
Reference = C3;
ValeurCmp = 100N;
IdModule  = ipc_capc:IPC_CAPC1005X55N;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53A8C6B1;
Reference = C4;
ValeurCmp = 100N;
IdModule  = ipc_capc:IPC_CAPC1005X55N;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53A8C6AB;
Reference = C5;
ValeurCmp = 100N;
IdModule  = ipc_capc:IPC_CAPC1005X55N;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53A8C687;
Reference = C6;
ValeurCmp = 100N;
IdModule  = ipc_capc:IPC_CAPC1005X55N;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53A8C70E;
Reference = C7;
ValeurCmp = 10U;
IdModule  = ipc_capc:IPC_CAPC2012X140N;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53A8C6F6;
Reference = C8;
ValeurCmp = 10U;
IdModule  = ipc_capc:IPC_CAPC2012X140N;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53A8C708;
Reference = C9;
ValeurCmp = 10U;
IdModule  = ipc_capc:IPC_CAPC2012X140N;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53A8C68D;
Reference = C10;
ValeurCmp = 100N;
IdModule  = ipc_capc:IPC_CAPC1005X55N;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53A8C72C;
Reference = C11;
ValeurCmp = 10U;
IdModule  = ipc_capc:IPC_CAPC2012X140N;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53A8C6F0;
Reference = C12;
ValeurCmp = 10U;
IdModule  = ipc_capc:IPC_CAPC2012X140N;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53A8C720;
Reference = C13;
ValeurCmp = 10U;
IdModule  = ipc_capc:IPC_CAPC2012X140N;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53AF1137;
Reference = C14;
ValeurCmp = 220P;
IdModule  = ipc_capc:IPC_CAPC1608X95N;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53AF112C;
Reference = C15;
ValeurCmp = 220P;
IdModule  = ipc_capc:IPC_CAPC1608X95N;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53AF15D9;
Reference = C16;
ValeurCmp = 1U;
IdModule  = ipc_capae:IPC_CAPAE430X540N;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53AF15E8;
Reference = C17;
ValeurCmp = 1U;
IdModule  = ipc_capae:IPC_CAPAE430X540N;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53A8C256;
Reference = C18;
ValeurCmp = 220U;
IdModule  = ipc_capae:IPC_CAPAE830X620N;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53A8C25E;
Reference = C19;
ValeurCmp = 220U;
IdModule  = ipc_capae:IPC_CAPAE830X620N;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53AF2762;
Reference = C20;
ValeurCmp = 10U;
IdModule  = ipc_capae:IPC_CAPAE430X540N;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53AF2753;
Reference = C21;
ValeurCmp = 10U;
IdModule  = ipc_capae:IPC_CAPAE430X540N;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53A8C27E;
Reference = C22;
ValeurCmp = 220P;
IdModule  = ipc_capc:IPC_CAPC1608X95N;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53A8C284;
Reference = C23;
ValeurCmp = 220P;
IdModule  = ipc_capc:IPC_CAPC1608X95N;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53A8C2AA;
Reference = C24;
ValeurCmp = 1U;
IdModule  = ipc_capae:IPC_CAPAE430X540N;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53A8C2A2;
Reference = C25;
ValeurCmp = 220P;
IdModule  = ipc_capc:IPC_CAPC1608X95N;
EndCmp

BeginCmp
TimeStamp = /53A9129D/53A8C71C;
Reference = C26;
ValeurCmp = 10U;
IdModule  = ipc_capc:IPC_CAPC2012X140N;
EndCmp

BeginCmp
TimeStamp = /53A9129D/53AA73CE;
Reference = C27;
ValeurCmp = 100N;
IdModule  = ipc_capc:IPC_CAPC1005X55N;
EndCmp

BeginCmp
TimeStamp = /53A8C780/53A8D527;
Reference = C28;
ValeurCmp = 100N;
IdModule  = ipc_capc:IPC_CAPC1005X55N;
EndCmp

BeginCmp
TimeStamp = /53A8C780/53A8D548;
Reference = C29;
ValeurCmp = 100N;
IdModule  = ipc_capc:IPC_CAPC1005X55N;
EndCmp

BeginCmp
TimeStamp = /53A8C780/53A8D542;
Reference = C30;
ValeurCmp = 100N;
IdModule  = ipc_capc:IPC_CAPC1005X55N;
EndCmp

BeginCmp
TimeStamp = /53A8C780/53A8D54E;
Reference = C31;
ValeurCmp = 100N;
IdModule  = ipc_capc:IPC_CAPC1005X55N;
EndCmp

BeginCmp
TimeStamp = /53A8C780/53A8D5C2;
Reference = C32;
ValeurCmp = 10U;
IdModule  = ipc_capc:IPC_CAPC2012X140N;
EndCmp

BeginCmp
TimeStamp = /53A8C780/53A8D56C;
Reference = C33;
ValeurCmp = 100N;
IdModule  = ipc_capc:IPC_CAPC1005X55N;
EndCmp

BeginCmp
TimeStamp = /53A8C780/53A8D5C8;
Reference = C34;
ValeurCmp = 10U;
IdModule  = ipc_capc:IPC_CAPC2012X140N;
EndCmp

BeginCmp
TimeStamp = /53A8C780/53A8D572;
Reference = C35;
ValeurCmp = 100N;
IdModule  = ipc_capc:IPC_CAPC1005X55N;
EndCmp

BeginCmp
TimeStamp = /53A8C780/53A8D5DA;
Reference = C36;
ValeurCmp = 10U;
IdModule  = ipc_capc:IPC_CAPC2012X140N;
EndCmp

BeginCmp
TimeStamp = /53A8C780/53A8D5E0;
Reference = C37;
ValeurCmp = 10U;
IdModule  = ipc_capc:IPC_CAPC2012X140N;
EndCmp

BeginCmp
TimeStamp = /53A8C780/53A8D58C;
Reference = C38;
ValeurCmp = 10U;
IdModule  = ipc_capc:IPC_CAPC2012X140N;
EndCmp

BeginCmp
TimeStamp = /53A8C780/53A8D5AA;
Reference = C39;
ValeurCmp = DNI;
IdModule  = ipc_capc:IPC_CAPC1608X90N;
EndCmp

BeginCmp
TimeStamp = /53A8C780/53A8D592;
Reference = C40;
ValeurCmp = 10U;
IdModule  = ipc_capc:IPC_CAPC2012X140N;
EndCmp

BeginCmp
TimeStamp = /53A8C780/53A8D62C;
Reference = C41;
ValeurCmp = 10U;
IdModule  = ipc_capc:IPC_CAPC2012X140N;
EndCmp

BeginCmp
TimeStamp = /53A8C780/53B1911F;
Reference = C42;
ValeurCmp = 10U;
IdModule  = ipc_capc:IPC_CAPC2012X140N;
EndCmp

BeginCmp
TimeStamp = /53A8C780/53B1A065;
Reference = C43;
ValeurCmp = 10U;
IdModule  = ipc_capc:IPC_CAPC2012X140N;
EndCmp

BeginCmp
TimeStamp = /53B309AC;
Reference = FID1;
ValeurCmp = FIDUCIAL;
IdModule  = fiducial:FIDUCIAL_65MIL;
EndCmp

BeginCmp
TimeStamp = /53B30B4C;
Reference = FID2;
ValeurCmp = FIDUCIAL;
IdModule  = fiducial:FIDUCIAL_65MIL;
EndCmp

BeginCmp
TimeStamp = /53B30CEC;
Reference = FID3;
ValeurCmp = FIDUCIAL;
IdModule  = fiducial:FIDUCIAL_65MIL;
EndCmp

BeginCmp
TimeStamp = /53B30E8C;
Reference = FID4;
ValeurCmp = FIDUCIAL;
IdModule  = fiducial:FIDUCIAL_65MIL;
EndCmp

BeginCmp
TimeStamp = /5369BBC4;
Reference = H1;
ValeurCmp = HOLE1;
IdModule  = hole:HOLE_3200UM_VIAS;
EndCmp

BeginCmp
TimeStamp = /5369BBD8;
Reference = H2;
ValeurCmp = HOLE1;
IdModule  = hole:HOLE_3200UM_VIAS;
EndCmp

BeginCmp
TimeStamp = /5369BBEC;
Reference = H3;
ValeurCmp = HOLE1;
IdModule  = hole:HOLE_3200UM_VIAS;
EndCmp

BeginCmp
TimeStamp = /5369BC00;
Reference = H4;
ValeurCmp = HOLE1;
IdModule  = hole:HOLE_3200UM_VIAS;
EndCmp

BeginCmp
TimeStamp = /5369BC14;
Reference = H5;
ValeurCmp = HOLE1;
IdModule  = hole:HOLE_3200UM_VIAS;
EndCmp

BeginCmp
TimeStamp = /53A9129D/53A8C6D0;
Reference = J2;
ValeurCmp = MICROSD_DETSW;
IdModule  = alps:ALPS_SCHA4B0100;
EndCmp

BeginCmp
TimeStamp = /53A9129D/53A91651;
Reference = J3;
ValeurCmp = KINGTECH_DW0240A2BZ_FPC;
IdModule  = molex:MOLEX_54132-40XX_LR;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53AF093C;
Reference = L1;
ValeurCmp = L;
IdModule  = ipc_indc:IPC_INDC1608X95N;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53AF20F3;
Reference = L2;
ValeurCmp = L;
IdModule  = ipc_indc:IPC_INDC1608X95N;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53AF20FE;
Reference = L3;
ValeurCmp = L;
IdModule  = ipc_indc:IPC_INDC1608X95N;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53A8C2E2;
Reference = L4;
ValeurCmp = L;
IdModule  = ipc_indc:IPC_INDC1608X95N;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53A8C2E8;
Reference = L5;
ValeurCmp = L;
IdModule  = ipc_indc:IPC_INDC1608X95N;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53A8C2EE;
Reference = L6;
ValeurCmp = L;
IdModule  = ipc_indc:IPC_INDC1608X95N;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53AF25CC;
Reference = L7;
ValeurCmp = L;
IdModule  = ipc_indc:IPC_INDC1608X95N;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53AF25D7;
Reference = L8;
ValeurCmp = L;
IdModule  = ipc_indc:IPC_INDC1608X95N;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53A8C2F4;
Reference = L9;
ValeurCmp = L;
IdModule  = ipc_indc:IPC_INDC1608X95N;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53AF0931;
Reference = L10;
ValeurCmp = L;
IdModule  = ipc_indc:IPC_INDC1608X95N;
EndCmp

BeginCmp
TimeStamp = /53A9129D/53A8C752;
Reference = LCD1;
ValeurCmp = KINGTECH_DW0240A2BZ_PANEL;
IdModule  = lcd_kingtech:KINGTECH_DW0240A2BZ_PANEL;
EndCmp

BeginCmp
TimeStamp = /53B1AE0D;
Reference = LOGO1;
ValeurCmp = SHAREBRAINED;
IdModule  = sharebrained:sharebrained_text_300;
EndCmp

BeginCmp
TimeStamp = /53B1B509;
Reference = LOGO2;
ValeurCmp = PORTAPACK_H1;
IdModule  = sharebrained:portapack_text_300;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53AF0914;
Reference = P1;
ValeurCmp = TRS_JACK;
IdModule  = cui:CUI_SJ-3524-SMT;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53A8C2C6;
Reference = P2;
ValeurCmp = TRRS_SW_JACK;
IdModule  = cui:CUI_SJ-43516-SMT;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53AF0926;
Reference = P3;
ValeurCmp = TRS_JACK;
IdModule  = cui:CUI_SJ-3524-SMT;
EndCmp

BeginCmp
TimeStamp = /53A8C780/53A8CDAE;
Reference = P20;
ValeurCmp = HACKRF_ONE_P20;
IdModule  = header:HEADER_11X2_REV_SM_254_AP;
EndCmp

BeginCmp
TimeStamp = /53A8C780/53A8CDB6;
Reference = P22;
ValeurCmp = HACKRF_ONE_P22;
IdModule  = header:HEADER_13X2_REV_SM_254_AP;
EndCmp

BeginCmp
TimeStamp = /53A8C780/53A8CDBE;
Reference = P28;
ValeurCmp = HACKRF_ONE_P28;
IdModule  = header:HEADER_11X2_REV_SM_254_AP;
EndCmp

BeginCmp
TimeStamp = /53A9129D/53C5B6EB;
Reference = Q1;
ValeurCmp = MOSFET_N;
IdModule  = ipc_sot:IPC_SOT95P230X110-3N;
EndCmp

BeginCmp
TimeStamp = /53A8C780/53AB79CA;
Reference = R1;
ValeurCmp = 220R;
IdModule  = ipc_resc:IPC_RESC1608X55N;
EndCmp

BeginCmp
TimeStamp = /53A8C780/53AB79D5;
Reference = R2;
ValeurCmp = 220R;
IdModule  = ipc_resc:IPC_RESC1608X55N;
EndCmp

BeginCmp
TimeStamp = /53A8C780/53AB79EA;
Reference = R3;
ValeurCmp = 220R;
IdModule  = ipc_resc:IPC_RESC1608X55N;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53AF0B7F;
Reference = R6;
ValeurCmp = 5K6;
IdModule  = ipc_resc:IPC_RESC1608X55N;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53AF0B74;
Reference = R7;
ValeurCmp = 5K6;
IdModule  = ipc_resc:IPC_RESC1608X55N;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53AF0B8A;
Reference = R8;
ValeurCmp = 5K6;
IdModule  = ipc_resc:IPC_RESC1608X55N;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53AF0B95;
Reference = R9;
ValeurCmp = 5K6;
IdModule  = ipc_resc:IPC_RESC1608X55N;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53A8C2B0;
Reference = R10;
ValeurCmp = 47K;
IdModule  = ipc_resc:IPC_RESC1608X55N;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53A8C264;
Reference = R11;
ValeurCmp = 47K;
IdModule  = ipc_resc:IPC_RESC1608X55N;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53A8C26A;
Reference = R12;
ValeurCmp = 47K;
IdModule  = ipc_resc:IPC_RESC1608X55N;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53AF2746;
Reference = R13;
ValeurCmp = 47K;
IdModule  = ipc_resc:IPC_RESC1608X55N;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53AF273B;
Reference = R14;
ValeurCmp = 47K;
IdModule  = ipc_resc:IPC_RESC1608X55N;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53AF2725;
Reference = R15;
ValeurCmp = 100R;
IdModule  = ipc_resc:IPC_RESC1608X55N;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53AF2730;
Reference = R16;
ValeurCmp = 100R;
IdModule  = ipc_resc:IPC_RESC1608X55N;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53A8C296;
Reference = R17;
ValeurCmp = 47K;
IdModule  = ipc_resc:IPC_RESC1608X55N;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53A8C29C;
Reference = R18;
ValeurCmp = 680R;
IdModule  = ipc_resc:IPC_RESC1608X55N;
EndCmp

BeginCmp
TimeStamp = /53A9129D/53A91657;
Reference = R19;
ValeurCmp = 47K;
IdModule  = ipc_resc:IPC_RESC1608X55N;
EndCmp

BeginCmp
TimeStamp = /53A9129D/53A91635;
Reference = R20;
ValeurCmp = 47K;
IdModule  = ipc_resc:IPC_RESC1608X55N;
EndCmp

BeginCmp
TimeStamp = /53A8C780/53A915E9;
Reference = R22;
ValeurCmp = 220R;
IdModule  = ipc_resc:IPC_RESC1608X55N;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53AB09AD;
Reference = RP1;
ValeurCmp = 220R;
IdModule  = ipc_resc:IPC_RESCAXS80P160X320X60-8N;
EndCmp

BeginCmp
TimeStamp = /53A8C780/53AB047A;
Reference = RP4;
ValeurCmp = 220R;
IdModule  = ipc_resc:IPC_RESCAXS80P160X320X60-8N;
EndCmp

BeginCmp
TimeStamp = /53A8C780/53AB04B9;
Reference = RP6;
ValeurCmp = 220R;
IdModule  = ipc_resc:IPC_RESCAXS80P160X320X60-8N;
EndCmp

BeginCmp
TimeStamp = /53A8C780/53AB04D6;
Reference = RP7;
ValeurCmp = 220R;
IdModule  = ipc_resc:IPC_RESCAXS80P160X320X60-8N;
EndCmp

BeginCmp
TimeStamp = /53A9129D/53A8C6FD;
Reference = SW1;
ValeurCmp = CK_TSWB-3N-CB;
IdModule  = ck:CK_TSWB-3N-CB222_LFS;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53A8C66D;
Reference = U1;
ValeurCmp = WM8731SEDS;
IdModule  = ipc_sop:IPC_SOP65P780X200-28N;
EndCmp

BeginCmp
TimeStamp = /53A8C780/53A8D586;
Reference = U2;
ValeurCmp = REGULATOR_SOT23_5;
IdModule  = ipc_sot:IPC_SOT95P280X110-5N;
EndCmp

BeginCmp
TimeStamp = /53A8C780/53A8D11B;
Reference = U3;
ValeurCmp = 5M40ZE64;
IdModule  = ipc_qfp:IPC_QFP40P900X900X120-65N;
EndCmp

BeginCmp
TimeStamp = /53A8BFC3/53A8C2D6;
Reference = X1;
ValeurCmp = MIC_ELECTRET;
IdModule  = cui:CUI_CMA-4544PF-W;
EndCmp

EndListe
