(export (version D)
  (design
    (source portapack_h1.sch)
    (date "Thursday, July 17, 2014 'AMt' 08:44:16 AM")
    (tool "eeschema (2014-03-01 BZR 4730)-product"))
  (components
    (comp (ref H1)
      (value HOLE1)
      (libsource (lib hole) (part HOLE1))
      (sheetpath (names /) (tstamps /))
      (tstamp 5369BBC4))
    (comp (ref H2)
      (value HOLE1)
      (libsource (lib hole) (part HOLE1))
      (sheetpath (names /) (tstamps /))
      (tstamp 5369BBD8))
    (comp (ref H3)
      (value HOLE1)
      (libsource (lib hole) (part HOLE1))
      (sheetpath (names /) (tstamps /))
      (tstamp 5369BBEC))
    (comp (ref H4)
      (value HOLE1)
      (libsource (lib hole) (part HOLE1))
      (sheetpath (names /) (tstamps /))
      (tstamp 5369BC00))
    (comp (ref H5)
      (value HOLE1)
      (libsource (lib hole) (part HOLE1))
      (sheetpath (names /) (tstamps /))
      (tstamp 5369BC14))
    (comp (ref LOGO1)
      (value SHAREBRAINED)
      (libsource (lib sharebrained) (part SHAREBRAINED))
      (sheetpath (names /) (tstamps /))
      (tstamp 53B1AE0D))
    (comp (ref LOGO2)
      (value PORTAPACK_H1)
      (libsource (lib sharebrained) (part PORTAPACK_H1))
      (sheetpath (names /) (tstamps /))
      (tstamp 53B1B509))
    (comp (ref FID1)
      (value FIDUCIAL)
      (libsource (lib fiducial) (part FIDUCIAL))
      (sheetpath (names /) (tstamps /))
      (tstamp 53B309AC))
    (comp (ref FID2)
      (value FIDUCIAL)
      (libsource (lib fiducial) (part FIDUCIAL))
      (sheetpath (names /) (tstamps /))
      (tstamp 53B30B4C))
    (comp (ref FID3)
      (value FIDUCIAL)
      (libsource (lib fiducial) (part FIDUCIAL))
      (sheetpath (names /) (tstamps /))
      (tstamp 53B30CEC))
    (comp (ref FID4)
      (value FIDUCIAL)
      (libsource (lib fiducial) (part FIDUCIAL))
      (sheetpath (names /) (tstamps /))
      (tstamp 53B30E8C))
    (comp (ref C18)
      (value 220U)
      (fields
        (field (name Mfr) Nichicon)
        (field (name Part) UWX1A221MCL1GB))
      (libsource (lib passive) (part CP))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53A8C256))
    (comp (ref C19)
      (value 220U)
      (fields
        (field (name Mfr) Nichicon)
        (field (name Part) UWX1A221MCL1GB))
      (libsource (lib passive) (part CP))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53A8C25E))
    (comp (ref R11)
      (value 47K)
      (fields
        (field (name Mfr) Yageo)
        (field (name Part) RC0603FR-0747KL))
      (libsource (lib passive) (part R))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53A8C264))
    (comp (ref R12)
      (value 47K)
      (fields
        (field (name Mfr) Yageo)
        (field (name Part) RC0603FR-0747KL))
      (libsource (lib passive) (part R))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53A8C26A))
    (comp (ref C22)
      (value 220P)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM1885C1H221JA01))
      (libsource (lib passive) (part C))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53A8C27E))
    (comp (ref C23)
      (value 220P)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM1885C1H221JA01))
      (libsource (lib passive) (part C))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53A8C284))
    (comp (ref R17)
      (value 47K)
      (fields
        (field (name Mfr) Yageo)
        (field (name Part) RC0603FR-0747KL))
      (libsource (lib passive) (part R))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53A8C296))
    (comp (ref R18)
      (value 680R)
      (libsource (lib passive) (part R))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53A8C29C))
    (comp (ref C25)
      (value 220P)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM1885C1H221JA01))
      (libsource (lib passive) (part C))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53A8C2A2))
    (comp (ref C24)
      (value 1U)
      (fields
        (field (name Mfr) Kemet)
        (field (name Part) EDK105M050A9BAA))
      (libsource (lib passive) (part CP))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53A8C2AA))
    (comp (ref R10)
      (value 47K)
      (fields
        (field (name Mfr) Yageo)
        (field (name Part) RC0603FR-0747KL))
      (libsource (lib passive) (part R))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53A8C2B0))
    (comp (ref P2)
      (value TRRS_SW_JACK)
      (fields
        (field (name Mfr) CUI)
        (field (name Part) SJ-43514-SMT))
      (libsource (lib trs_jack) (part TRRS_SW_JACK))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53A8C2C6))
    (comp (ref X1)
      (value MIC_ELECTRET)
      (fields
        (field (name Mfr) CUI)
        (field (name Part) CMA-4544PF-W))
      (libsource (lib microphone) (part MIC_ELECTRET))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53A8C2D6))
    (comp (ref L4)
      (value L)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) BLM18HE152SN1D))
      (libsource (lib passive) (part L))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53A8C2E2))
    (comp (ref L5)
      (value L)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) BLM18HE152SN1D))
      (libsource (lib passive) (part L))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53A8C2E8))
    (comp (ref L6)
      (value L)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) BLM18HE152SN1D))
      (libsource (lib passive) (part L))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53A8C2EE))
    (comp (ref L9)
      (value L)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) BLM18HE152SN1D))
      (libsource (lib passive) (part L))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53A8C2F4))
    (comp (ref U1)
      (value WM8731SEDS)
      (fields
        (field (name Mfr) Wolfson)
        (field (name Part) WM8731SEDS/V))
      (libsource (lib wolfson) (part WM8731SEDS))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53A8C66D))
    (comp (ref C6)
      (value 100N)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM155R61A104KA01))
      (libsource (lib passive) (part C))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53A8C687))
    (comp (ref C10)
      (value 100N)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM155R61A104KA01))
      (libsource (lib passive) (part C))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53A8C68D))
    (comp (ref C3)
      (value 100N)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM155R61A104KA01))
      (libsource (lib passive) (part C))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53A8C69F))
    (comp (ref C2)
      (value 100N)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM155R61A104KA01))
      (libsource (lib passive) (part C))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53A8C6A5))
    (comp (ref C5)
      (value 100N)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM155R61A104KA01))
      (libsource (lib passive) (part C))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53A8C6AB))
    (comp (ref C4)
      (value 100N)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM155R61A104KA01))
      (libsource (lib passive) (part C))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53A8C6B1))
    (comp (ref C12)
      (value 10U)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM21BR61A106KE19))
      (libsource (lib passive) (part C))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53A8C6F0))
    (comp (ref C8)
      (value 10U)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM21BR61A106KE19))
      (libsource (lib passive) (part C))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53A8C6F6))
    (comp (ref C9)
      (value 10U)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM21BR61A106KE19))
      (libsource (lib passive) (part C))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53A8C708))
    (comp (ref C7)
      (value 10U)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM21BR61A106KE19))
      (libsource (lib passive) (part C))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53A8C70E))
    (comp (ref C13)
      (value 10U)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM21BR61A106KE19))
      (libsource (lib passive) (part C))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53A8C720))
    (comp (ref C11)
      (value 10U)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM21BR61A106KE19))
      (libsource (lib passive) (part C))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53A8C72C))
    (comp (ref RP1)
      (value 220R)
      (fields
        (field (name Mfr) Panasonic)
        (field (name Part) EXB-38V221JV))
      (libsource (lib passive) (part RPACK4))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53AB09AD))
    (comp (ref P1)
      (value TRS_JACK)
      (fields
        (field (name Mfr) Switchcraft)
        (field (name Part) 35RASMT2BHNTRX))
      (libsource (lib trs_jack) (part TRS_JACK))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53AF0914))
    (comp (ref P3)
      (value TRS_JACK)
      (fields
        (field (name Mfr) Switchcraft)
        (field (name Part) 35RASMT2BHNTRX))
      (libsource (lib trs_jack) (part TRS_JACK))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53AF0926))
    (comp (ref L10)
      (value L)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) BLM18HE152SN1D))
      (libsource (lib passive) (part L))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53AF0931))
    (comp (ref L1)
      (value L)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) BLM18HE152SN1D))
      (libsource (lib passive) (part L))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53AF093C))
    (comp (ref R7)
      (value 5K6)
      (fields
        (field (name Mfr) Yageo)
        (field (name Part) RC0603FR-075K6L))
      (libsource (lib passive) (part R))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53AF0B74))
    (comp (ref R6)
      (value 5K6)
      (fields
        (field (name Mfr) Yageo)
        (field (name Part) RC0603FR-075K6L))
      (libsource (lib passive) (part R))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53AF0B7F))
    (comp (ref R8)
      (value 5K6)
      (fields
        (field (name Mfr) Yageo)
        (field (name Part) RC0603FR-075K6L))
      (libsource (lib passive) (part R))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53AF0B8A))
    (comp (ref R9)
      (value 5K6)
      (fields
        (field (name Mfr) Yageo)
        (field (name Part) RC0603FR-075K6L))
      (libsource (lib passive) (part R))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53AF0B95))
    (comp (ref C15)
      (value 220P)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM1885C1H221JA01))
      (libsource (lib passive) (part C))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53AF112C))
    (comp (ref C14)
      (value 220P)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM1885C1H221JA01))
      (libsource (lib passive) (part C))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53AF1137))
    (comp (ref C16)
      (value 1U)
      (fields
        (field (name Mfr) Kemet)
        (field (name Part) EDK105M050A9BAA))
      (libsource (lib passive) (part CP))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53AF15D9))
    (comp (ref C17)
      (value 1U)
      (fields
        (field (name Mfr) Kemet)
        (field (name Part) EDK105M050A9BAA))
      (libsource (lib passive) (part CP))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53AF15E8))
    (comp (ref L2)
      (value L)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) BLM18HE152SN1D))
      (libsource (lib passive) (part L))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53AF20F3))
    (comp (ref L3)
      (value L)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) BLM18HE152SN1D))
      (libsource (lib passive) (part L))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53AF20FE))
    (comp (ref L7)
      (value L)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) BLM18HE152SN1D))
      (libsource (lib passive) (part L))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53AF25CC))
    (comp (ref L8)
      (value L)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) BLM18HE152SN1D))
      (libsource (lib passive) (part L))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53AF25D7))
    (comp (ref R15)
      (value 100R)
      (fields
        (field (name Mfr) Yageo)
        (field (name Part) RC0603FR-07100RL))
      (libsource (lib passive) (part R))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53AF2725))
    (comp (ref R16)
      (value 100R)
      (fields
        (field (name Mfr) Yageo)
        (field (name Part) RC0603FR-07100RL))
      (libsource (lib passive) (part R))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53AF2730))
    (comp (ref R14)
      (value 47K)
      (fields
        (field (name Mfr) Yageo)
        (field (name Part) RC0603FR-0747KL))
      (libsource (lib passive) (part R))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53AF273B))
    (comp (ref R13)
      (value 47K)
      (fields
        (field (name Mfr) Yageo)
        (field (name Part) RC0603FR-0747KL))
      (libsource (lib passive) (part R))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53AF2746))
    (comp (ref C21)
      (value 10U)
      (fields
        (field (name Mfr) Kemet)
        (field (name Part) EDK106M025A9BAA))
      (libsource (lib passive) (part CP))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53AF2753))
    (comp (ref C20)
      (value 10U)
      (fields
        (field (name Mfr) Kemet)
        (field (name Part) EDK106M025A9BAA))
      (libsource (lib passive) (part CP))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53AF2762))
    (comp (ref R20)
      (value 47K)
      (fields
        (field (name Mfr) Yageo)
        (field (name Part) RC0603FR-0747KL))
      (libsource (lib passive) (part R))
      (sheetpath (names /lcd_sw_sd/) (tstamps /53A9129D/))
      (tstamp 53A91635))
    (comp (ref J3)
      (value KINGTECH_DW0240A2BZ_FPC)
      (fields
        (field (name Mfr) FCI)
        (field (name Part) 62684-401100ALF))
      (libsource (lib lcd_kingtech) (part KINGTECH_DW0240A2BZ_FPC))
      (sheetpath (names /lcd_sw_sd/) (tstamps /53A9129D/))
      (tstamp 53A91651))
    (comp (ref R19)
      (value 47K)
      (fields
        (field (name Mfr) Yageo)
        (field (name Part) RC0603FR-0747KL))
      (libsource (lib passive) (part R))
      (sheetpath (names /lcd_sw_sd/) (tstamps /53A9129D/))
      (tstamp 53A91657))
    (comp (ref J2)
      (value MICROSD_DETSW)
      (fields
        (field (name Mfr) ALPS)
        (field (name Part) SCHA4B0100))
      (libsource (lib sd) (part MICROSD_DETSW))
      (sheetpath (names /lcd_sw_sd/) (tstamps /53A9129D/))
      (tstamp 53A8C6D0))
    (comp (ref C27)
      (value 100N)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM155R61A104KA01))
      (libsource (lib passive) (part C))
      (sheetpath (names /lcd_sw_sd/) (tstamps /53A9129D/))
      (tstamp 53AA73CE))
    (comp (ref SW1)
      (value CK_TSWB-3N-CB)
      (fields
        (field (name Mfr) C&K)
        (field (name Part) "TSWB-3N-CB111 LFS"))
      (libsource (lib ck) (part CK_TSWB-3N-CB))
      (sheetpath (names /lcd_sw_sd/) (tstamps /53A9129D/))
      (tstamp 53A8C6FD))
    (comp (ref C26)
      (value 10U)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM21BR61A106KE19))
      (libsource (lib passive) (part C))
      (sheetpath (names /lcd_sw_sd/) (tstamps /53A9129D/))
      (tstamp 53A8C71C))
    (comp (ref LCD1)
      (value KINGTECH_DW0240A2BZ_PANEL)
      (libsource (lib lcd_kingtech) (part KINGTECH_DW0240A2BZ_PANEL))
      (sheetpath (names /lcd_sw_sd/) (tstamps /53A9129D/))
      (tstamp 53A8C752))
    (comp (ref Q1)
      (value MOSFET_N)
      (fields
        (field (name Mfr) NXP)
        (field (name Part) 2N7002P,215))
      (libsource (lib mosfet) (part MOSFET_N))
      (sheetpath (names /lcd_sw_sd/) (tstamps /53A9129D/))
      (tstamp 53C5B6EB))
    (comp (ref P20)
      (value HACKRF_ONE_P20)
      (fields
        (field (name Mfr) Harwin)
        (field (name Part) M20-8761146))
      (libsource (lib hackrf_expansion) (part HACKRF_ONE_P20))
      (sheetpath (names /hackrf_if/) (tstamps /53A8C780/))
      (tstamp 53A8CDAE))
    (comp (ref P22)
      (value HACKRF_ONE_P22)
      (fields
        (field (name Mfr) Harwin)
        (field (name Part) M20-8761346))
      (libsource (lib hackrf_expansion) (part HACKRF_ONE_P22))
      (sheetpath (names /hackrf_if/) (tstamps /53A8C780/))
      (tstamp 53A8CDB6))
    (comp (ref P28)
      (value HACKRF_ONE_P28)
      (fields
        (field (name Mfr) Harwin)
        (field (name Part) M20-8761146))
      (libsource (lib hackrf_expansion) (part HACKRF_ONE_P28))
      (sheetpath (names /hackrf_if/) (tstamps /53A8C780/))
      (tstamp 53A8CDBE))
    (comp (ref U3)
      (value 5M40ZE64)
      (fields
        (field (name Mfr) Altera)
        (field (name Part) 5M40ZE64C5N))
      (libsource (lib altera) (part 5M40ZE64))
      (sheetpath (names /hackrf_if/) (tstamps /53A8C780/))
      (tstamp 53A8D11B))
    (comp (ref C28)
      (value 100N)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM155R61A104KA01))
      (libsource (lib passive) (part C))
      (sheetpath (names /hackrf_if/) (tstamps /53A8C780/))
      (tstamp 53A8D527))
    (comp (ref BT1)
      (value BATTERY)
      (fields
        (field (name Mfr) MPD)
        (field (name Part) BU2032SM-BT-GTR))
      (libsource (lib battery) (part BATTERY))
      (sheetpath (names /hackrf_if/) (tstamps /53A8C780/))
      (tstamp 53A8D535))
    (comp (ref C30)
      (value 100N)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM155R61A104KA01))
      (libsource (lib passive) (part C))
      (sheetpath (names /hackrf_if/) (tstamps /53A8C780/))
      (tstamp 53A8D542))
    (comp (ref C29)
      (value 100N)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM155R61A104KA01))
      (libsource (lib passive) (part C))
      (sheetpath (names /hackrf_if/) (tstamps /53A8C780/))
      (tstamp 53A8D548))
    (comp (ref C31)
      (value 100N)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM155R61A104KA01))
      (libsource (lib passive) (part C))
      (sheetpath (names /hackrf_if/) (tstamps /53A8C780/))
      (tstamp 53A8D54E))
    (comp (ref C33)
      (value 100N)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM155R61A104KA01))
      (libsource (lib passive) (part C))
      (sheetpath (names /hackrf_if/) (tstamps /53A8C780/))
      (tstamp 53A8D56C))
    (comp (ref C35)
      (value 100N)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM155R61A104KA01))
      (libsource (lib passive) (part C))
      (sheetpath (names /hackrf_if/) (tstamps /53A8C780/))
      (tstamp 53A8D572))
    (comp (ref U2)
      (value REGULATOR_SOT23_5)
      (fields
        (field (name Mfr) Toshiba)
        (field (name Part) TCR2EF18,LM))
      (libsource (lib regulator) (part REGULATOR_SOT23_5))
      (sheetpath (names /hackrf_if/) (tstamps /53A8C780/))
      (tstamp 53A8D586))
    (comp (ref C38)
      (value 10U)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM21BR61A106KE19))
      (libsource (lib passive) (part C))
      (sheetpath (names /hackrf_if/) (tstamps /53A8C780/))
      (tstamp 53A8D58C))
    (comp (ref C40)
      (value 10U)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM21BR61A106KE19))
      (libsource (lib passive) (part C))
      (sheetpath (names /hackrf_if/) (tstamps /53A8C780/))
      (tstamp 53A8D592))
    (comp (ref C39)
      (value DNI)
      (libsource (lib passive) (part C))
      (sheetpath (names /hackrf_if/) (tstamps /53A8C780/))
      (tstamp 53A8D5AA))
    (comp (ref C32)
      (value 10U)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM21BR61A106KE19))
      (libsource (lib passive) (part C))
      (sheetpath (names /hackrf_if/) (tstamps /53A8C780/))
      (tstamp 53A8D5C2))
    (comp (ref C34)
      (value 10U)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM21BR61A106KE19))
      (libsource (lib passive) (part C))
      (sheetpath (names /hackrf_if/) (tstamps /53A8C780/))
      (tstamp 53A8D5C8))
    (comp (ref C36)
      (value 10U)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM21BR61A106KE19))
      (libsource (lib passive) (part C))
      (sheetpath (names /hackrf_if/) (tstamps /53A8C780/))
      (tstamp 53A8D5DA))
    (comp (ref C37)
      (value 10U)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM21BR61A106KE19))
      (libsource (lib passive) (part C))
      (sheetpath (names /hackrf_if/) (tstamps /53A8C780/))
      (tstamp 53A8D5E0))
    (comp (ref C41)
      (value 10U)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM21BR61A106KE19))
      (libsource (lib passive) (part C))
      (sheetpath (names /hackrf_if/) (tstamps /53A8C780/))
      (tstamp 53A8D62C))
    (comp (ref R22)
      (value 220R)
      (fields
        (field (name Mfr) Yageo)
        (field (name Part) RC0603FR-07220RL))
      (libsource (lib passive) (part R))
      (sheetpath (names /hackrf_if/) (tstamps /53A8C780/))
      (tstamp 53A915E9))
    (comp (ref RP4)
      (value 220R)
      (fields
        (field (name Mfr) Panasonic)
        (field (name Part) EXB-38V221JV))
      (libsource (lib passive) (part RPACK4))
      (sheetpath (names /hackrf_if/) (tstamps /53A8C780/))
      (tstamp 53AB047A))
    (comp (ref RP6)
      (value 220R)
      (fields
        (field (name Mfr) Panasonic)
        (field (name Part) EXB-38V221JV))
      (libsource (lib passive) (part RPACK4))
      (sheetpath (names /hackrf_if/) (tstamps /53A8C780/))
      (tstamp 53AB04B9))
    (comp (ref RP7)
      (value 220R)
      (fields
        (field (name Mfr) Panasonic)
        (field (name Part) EXB-38V221JV))
      (libsource (lib passive) (part RPACK4))
      (sheetpath (names /hackrf_if/) (tstamps /53A8C780/))
      (tstamp 53AB04D6))
    (comp (ref R1)
      (value 220R)
      (fields
        (field (name Mfr) Yageo)
        (field (name Part) RC0603FR-07220RL))
      (libsource (lib passive) (part R))
      (sheetpath (names /hackrf_if/) (tstamps /53A8C780/))
      (tstamp 53AB79CA))
    (comp (ref R2)
      (value 220R)
      (fields
        (field (name Mfr) Yageo)
        (field (name Part) RC0603FR-07220RL))
      (libsource (lib passive) (part R))
      (sheetpath (names /hackrf_if/) (tstamps /53A8C780/))
      (tstamp 53AB79D5))
    (comp (ref R3)
      (value 220R)
      (fields
        (field (name Mfr) Yageo)
        (field (name Part) RC0603FR-07220RL))
      (libsource (lib passive) (part R))
      (sheetpath (names /hackrf_if/) (tstamps /53A8C780/))
      (tstamp 53AB79EA))
    (comp (ref C42)
      (value 10U)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM21BR61A106KE19))
      (libsource (lib passive) (part C))
      (sheetpath (names /hackrf_if/) (tstamps /53A8C780/))
      (tstamp 53B1911F))
    (comp (ref C43)
      (value 10U)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM21BR61A106KE19))
      (libsource (lib passive) (part C))
      (sheetpath (names /hackrf_if/) (tstamps /53A8C780/))
      (tstamp 53B1A065)))
  (libparts
    (libpart (lib wolfson) (part WM8731SEDS)
      (footprints
        (fp IPC_SOP65P780X200-28N))
      (fields
        (field (name Reference) U)
        (field (name Value) WM8731SEDS))
      (pins
        (pin (num 1) (name DBVDD) (type power_in))
        (pin (num 2) (name CLKOUT) (type output))
        (pin (num 3) (name BCLK) (type BiDi))
        (pin (num 4) (name DACDAT) (type input))
        (pin (num 5) (name DACLRC) (type BiDi))
        (pin (num 6) (name ADCDAT) (type output))
        (pin (num 7) (name ADCLRC) (type BiDi))
        (pin (num 8) (name HPVDD) (type power_in))
        (pin (num 9) (name LHPOUT) (type output))
        (pin (num 10) (name RHPOUT) (type output))
        (pin (num 11) (name HPGND) (type power_in))
        (pin (num 12) (name LOUT) (type output))
        (pin (num 13) (name ROUT) (type output))
        (pin (num 14) (name AVDD) (type power_in))
        (pin (num 15) (name AGND) (type power_in))
        (pin (num 16) (name VMID) (type output))
        (pin (num 17) (name MICBIAS) (type output))
        (pin (num 18) (name MICIN) (type input))
        (pin (num 19) (name RLINEIN) (type input))
        (pin (num 20) (name LLINEIN) (type input))
        (pin (num 21) (name MODE) (type input))
        (pin (num 22) (name CSB) (type input))
        (pin (num 23) (name SDIN) (type BiDi))
        (pin (num 24) (name SCLK) (type input))
        (pin (num 25) (name XTI/MCLK) (type input))
        (pin (num 26) (name XTO) (type output))
        (pin (num 27) (name DCVDD) (type power_in))
        (pin (num 28) (name DGND) (type power_in))))
    (libpart (lib passive) (part C)
      (footprints
        (fp IPC_CAPC*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib passive) (part CP)
      (aliases
        (alias CAPAPOL))
      (footprints
        (fp IPC_CAPCP*)
        (fp IPC_CAPAE*)
        (fp IPC_CAPMP*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib passive) (part L)
      (footprints
        (fp IPC_INDC*))
      (fields
        (field (name Reference) L)
        (field (name Value) L))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib passive) (part R)
      (footprints
        (fp IPC_RESC*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib passive) (part RPACK4)
      (footprints
        (fp IPC_RESCAXS80P160X320X60-8N))
      (fields
        (field (name Reference) RP)
        (field (name Value) RPACK4))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))
        (pin (num 6) (name ~) (type passive))
        (pin (num 7) (name ~) (type passive))
        (pin (num 8) (name ~) (type passive))))
    (libpart (lib trs_jack) (part TRRS_SW_JACK)
      (footprints
        (fp CUI_SJ-43516-SMT))
      (fields
        (field (name Reference) P)
        (field (name Value) TRRS_SW_JACK))
      (pins
        (pin (num 1) (name S) (type passive))
        (pin (num 2) (name T) (type passive))
        (pin (num 3) (name R1) (type passive))
        (pin (num 4) (name R2) (type passive))
        (pin (num 5) (name TSW) (type passive))
        (pin (num 6) (name RSW) (type passive))))
    (libpart (lib trs_jack) (part TRS_JACK)
      (footprints
        (fp CUI_SJ1-352XN)
        (fp CUI_SJ-3523-SMT)
        (fp CUI_SJ-3524-SMT))
      (fields
        (field (name Reference) P)
        (field (name Value) TRS_JACK))
      (pins
        (pin (num 1) (name S) (type passive))
        (pin (num 2) (name T) (type passive))
        (pin (num 3) (name R) (type passive))))
    (libpart (lib battery) (part BATTERY)
      (footprints
        (fp MPD_BU2032SM-BT-G))
      (fields
        (field (name Reference) BT)
        (field (name Value) BATTERY))
      (pins
        (pin (num 1) (name +) (type passive))
        (pin (num 2) (name -) (type passive))))
    (libpart (lib mosfet) (part MOSFET_N)
      (footprints
        (fp IPC_SOT95P230X110-3N))
      (fields
        (field (name Reference) Q)
        (field (name Value) MOSFET_N))
      (pins
        (pin (num 1) (name G) (type passive))
        (pin (num 2) (name S) (type passive))
        (pin (num 3) (name D) (type passive))))
    (libpart (lib microphone) (part MIC_ELECTRET)
      (footprints
        (fp CUI_CMA-4544PF-W))
      (fields
        (field (name Reference) U)
        (field (name Value) MIC_ELECTRET))
      (pins
        (pin (num 1) (name +) (type output))
        (pin (num 2) (name -) (type output))))
    (libpart (lib sd) (part MICROSD_DETSW)
      (footprints
        (fp HIROSE_DM3D)
        (fp ALPS_SCHA4B0400))
      (fields
        (field (name Reference) J)
        (field (name Value) MICROSD_DETSW))
      (pins
        (pin (num 0) (name GND) (type power_in))
        (pin (num 1) (name DAT2) (type BiDi))
        (pin (num 2) (name DAT3/CD) (type BiDi))
        (pin (num 3) (name CMD) (type BiDi))
        (pin (num 4) (name VDD) (type power_in))
        (pin (num 5) (name CLK) (type input))
        (pin (num 6) (name VSS) (type power_in))
        (pin (num 7) (name DAT0) (type BiDi))
        (pin (num 8) (name DAT1) (type BiDi))
        (pin (num A) (name DETA) (type passive))
        (pin (num B) (name DETB) (type passive))
        (pin (num SH) (name SHIELD) (type passive))))
    (libpart (lib ck) (part CK_TSWB-3N-CB)
      (footprints
        (fp CK_TSWB-3N-CB*))
      (fields
        (field (name Reference) SW)
        (field (name Value) CK_TSWB-3N-CB))
      (pins
        (pin (num A) (name ROT_A) (type BiDi))
        (pin (num B) (name ROT_B) (type BiDi))
        (pin (num CA) (name COM_A) (type BiDi))
        (pin (num CB) (name COM_B) (type BiDi))
        (pin (num S1) (name SEL) (type BiDi))
        (pin (num S2) (name D) (type BiDi))
        (pin (num S3) (name R) (type BiDi))
        (pin (num S4) (name U) (type BiDi))
        (pin (num S5) (name L) (type BiDi))))
    (libpart (lib altera) (part 5M40ZE64)
      (footprints
        (fp IPC_QFP40P900X900X120-65N))
      (fields
        (field (name Reference) U)
        (field (name Value) 5M40ZE64))
      (pins
        (pin (num 1) (name IO/DIFFIO_L1n) (type BiDi))
        (pin (num 2) (name IO) (type BiDi))
        (pin (num 3) (name IO/DIFFIO_L2p) (type BiDi))
        (pin (num 4) (name IO/DIFFIO_L2n) (type BiDi))
        (pin (num 5) (name IO) (type BiDi))
        (pin (num 6) (name VCCIO1) (type power_in))
        (pin (num 7) (name IO/CLK0) (type BiDi))
        (pin (num 8) (name VCCINT) (type power_in))
        (pin (num 9) (name IO/CLK1) (type BiDi))
        (pin (num 10) (name IO) (type BiDi))
        (pin (num 11) (name IO/DIFFIO_L3p) (type BiDi))
        (pin (num 12) (name IO/DIFFIO_L3n) (type BiDi))
        (pin (num 13) (name IO) (type BiDi))
        (pin (num 14) (name TMS) (type input))
        (pin (num 15) (name TDI) (type input))
        (pin (num 16) (name TCK) (type input))
        (pin (num 17) (name TDO) (type output))
        (pin (num 18) (name IO/DIFFIO_B1p) (type BiDi))
        (pin (num 19) (name IO/DIFFIO_B1n) (type BiDi))
        (pin (num 20) (name IO/DIFFIO_B2p) (type BiDi))
        (pin (num 21) (name IO/DIFFIO_B2n) (type BiDi))
        (pin (num 22) (name IO/DIFFIO_B3p) (type BiDi))
        (pin (num 23) (name VCCIO1) (type power_in))
        (pin (num 24) (name IO/DIFFIO_B3n) (type BiDi))
        (pin (num 25) (name IO) (type BiDi))
        (pin (num 26) (name IO/DIFFIO_B4p) (type BiDi))
        (pin (num 27) (name IO/DIFFIO_B4n) (type BiDi))
        (pin (num 28) (name IO/DEV_OE/DIFFIO_B5p) (type BiDi))
        (pin (num 29) (name IO/DEV_CLRn/DIFFIO_B5n) (type BiDi))
        (pin (num 30) (name IO/DIFFIO_B6p) (type BiDi))
        (pin (num 31) (name IO/DIFFIO_B6n) (type BiDi))
        (pin (num 32) (name IO/DIFFIO_B7p) (type BiDi))
        (pin (num 33) (name IO/DIFFIO_B7n) (type BiDi))
        (pin (num 34) (name IO/DIFFIO_R4n) (type BiDi))
        (pin (num 35) (name IO/DIFFIO_R4p) (type BiDi))
        (pin (num 36) (name IO/DIFFIO_R3n) (type BiDi))
        (pin (num 37) (name IO/DIFFIO_R3p) (type BiDi))
        (pin (num 38) (name IO) (type BiDi))
        (pin (num 39) (name VCCIO2) (type power_in))
        (pin (num 40) (name IO/CLK2) (type BiDi))
        (pin (num 41) (name VCCINT) (type power_in))
        (pin (num 42) (name IO/CLK3) (type BiDi))
        (pin (num 43) (name IO/DIFFIO_R2n) (type BiDi))
        (pin (num 44) (name IO/DIFFIO_R2p) (type BiDi))
        (pin (num 45) (name IO) (type BiDi))
        (pin (num 46) (name IO/DIFFIO_R1n) (type BiDi))
        (pin (num 47) (name IO/DIFFIO_R1p) (type BiDi))
        (pin (num 48) (name IO) (type BiDi))
        (pin (num 49) (name IO/DIFFIO_T6n) (type BiDi))
        (pin (num 50) (name IO/DIFFIO_T6p) (type BiDi))
        (pin (num 51) (name IO) (type BiDi))
        (pin (num 52) (name IO/DIFFIO_T5n) (type BiDi))
        (pin (num 53) (name IO/DIFFIO_T5p) (type BiDi))
        (pin (num 54) (name IO/DIFFIO_T4n) (type BiDi))
        (pin (num 55) (name IO/DIFFIO_T4p) (type BiDi))
        (pin (num 56) (name IO/DIFFIO_T3n) (type BiDi))
        (pin (num 57) (name VCCIO2) (type power_in))
        (pin (num 58) (name IO/DIFFIO_T3p) (type BiDi))
        (pin (num 59) (name IO/DIFFIO_T2n) (type BiDi))
        (pin (num 60) (name IO/DIFFIO_T2p) (type BiDi))
        (pin (num 61) (name IO/DIFFIO_T1n) (type BiDi))
        (pin (num 62) (name IO) (type BiDi))
        (pin (num 63) (name IO/DIFFIO_T1p) (type BiDi))
        (pin (num 64) (name IO/DIFFIO_L1p) (type BiDi))
        (pin (num 65) (name GND) (type power_in))))
    (libpart (lib lcd_kingtech) (part KINGTECH_DW0240A2BZ_PANEL)
      (footprints
        (fp KINGTECH_DW0240A2BZ_PANEL))
      (fields
        (field (name Reference) LCD)
        (field (name Value) KINGTECH_DW0240A2BZ_PANEL)))
    (libpart (lib lcd_kingtech) (part KINGTECH_DW0240A2BZ_FPC)
      (footprints
        (fp MOLEX_54132-40XX_LR))
      (fields
        (field (name Reference) J)
        (field (name Value) KINGTECH_DW0240A2BZ_FPC))
      (pins
        (pin (num 1) (name LEDK) (type power_in))
        (pin (num 2) (name LEDA) (type power_in))
        (pin (num 3) (name GND) (type power_in))
        (pin (num 4) (name VCI) (type power_in))
        (pin (num 5) (name RESET#) (type input))
        (pin (num 6) (name RS/SCL) (type input))
        (pin (num 7) (name RD#) (type input))
        (pin (num 8) (name CS#) (type input))
        (pin (num 9) (name SDA) (type BiDi))
        (pin (num 10) (name WR#/DC) (type input))
        (pin (num 11) (name VSYNC) (type input))
        (pin (num 12) (name HSYNC) (type input))
        (pin (num 13) (name DOTCLK) (type input))
        (pin (num 14) (name DE) (type input))
        (pin (num 15) (name GND) (type power_in))
        (pin (num 16) (name DB17) (type BiDi))
        (pin (num 17) (name DB16) (type BiDi))
        (pin (num 18) (name DB15) (type BiDi))
        (pin (num 19) (name DB14) (type BiDi))
        (pin (num 20) (name DB13) (type BiDi))
        (pin (num 21) (name DB12) (type BiDi))
        (pin (num 22) (name DB11) (type BiDi))
        (pin (num 23) (name DB10) (type BiDi))
        (pin (num 24) (name DB9) (type BiDi))
        (pin (num 25) (name DB8) (type BiDi))
        (pin (num 26) (name DB7) (type BiDi))
        (pin (num 27) (name DB6) (type BiDi))
        (pin (num 28) (name DB5) (type BiDi))
        (pin (num 29) (name DB4) (type BiDi))
        (pin (num 30) (name DB3) (type BiDi))
        (pin (num 31) (name DB2) (type BiDi))
        (pin (num 32) (name DB1) (type BiDi))
        (pin (num 33) (name DB0) (type BiDi))
        (pin (num 34) (name TE) (type output))
        (pin (num 35) (name GND) (type power_in))
        (pin (num 36) (name IOVCC) (type power_in))
        (pin (num 37) (name TP_R) (type passive))
        (pin (num 38) (name TP_D) (type passive))
        (pin (num 39) (name TP_L) (type passive))
        (pin (num 40) (name TP_U) (type passive))
        (pin (num SHLD) (name ~) (type passive))))
    (libpart (lib hackrf_expansion) (part HACKRF_ONE_P20)
      (footprints
        (fp HEADER_11X2_*_254))
      (fields
        (field (name Reference) J)
        (field (name Value) HACKRF_ONE_P20))
      (pins
        (pin (num 1) (name VBAT) (type power_in))
        (pin (num 2) (name RTC_ALARM) (type output))
        (pin (num 3) (name VCC) (type power_out))
        (pin (num 4) (name WAKEUP) (type input))
        (pin (num 5) (name GPIO3_8) (type BiDi))
        (pin (num 6) (name GPIO3_9) (type BiDi))
        (pin (num 7) (name GPIO3_10) (type BiDi))
        (pin (num 8) (name GPIO3_11) (type BiDi))
        (pin (num 9) (name GPIO3_12) (type BiDi))
        (pin (num 10) (name GPIO3_13) (type BiDi))
        (pin (num 11) (name GPIO3_14) (type BiDi))
        (pin (num 12) (name GPIO3_15) (type BiDi))
        (pin (num 13) (name GND) (type power_in))
        (pin (num 14) (name ADC0_6) (type input))
        (pin (num 15) (name GND) (type power_in))
        (pin (num 16) (name ADC0_2) (type input))
        (pin (num 17) (name VBUSCTRL) (type input))
        (pin (num 18) (name ADC0_5) (type input))
        (pin (num 19) (name GND) (type power_in))
        (pin (num 20) (name ADC0_0) (type input))
        (pin (num 21) (name VBUS) (type output))
        (pin (num 22) (name VIN) (type power_in))))
    (libpart (lib hackrf_expansion) (part HACKRF_ONE_P22)
      (footprints
        (fp HEADER_13X2_*_254))
      (fields
        (field (name Reference) J)
        (field (name Value) HACKRF_ONE_P22))
      (pins
        (pin (num 1) (name CLKOUT) (type output))
        (pin (num 2) (name CLKIN) (type input))
        (pin (num 3) (name RESET#) (type output))
        (pin (num 4) (name GND) (type power_in))
        (pin (num 5) (name I2C1_SCL) (type output))
        (pin (num 6) (name I2C1_SDA) (type BiDi))
        (pin (num 7) (name SPIFI_MISO) (type input))
        (pin (num 8) (name SPIFI_SCK) (type output))
        (pin (num 9) (name SPIFI_MOSI) (type output))
        (pin (num 10) (name GND) (type power_in))
        (pin (num 11) (name VCC) (type power_out))
        (pin (num 12) (name I2S0_RX_SCK) (type output))
        (pin (num 13) (name I2S0_RX_SDA) (type input))
        (pin (num 14) (name I2S0_RX_MCLK) (type output))
        (pin (num 15) (name I2S0_RX_WS) (type output))
        (pin (num 16) (name I2S0_TX_SCK) (type output))
        (pin (num 17) (name I2S0_TX_MCLK) (type output))
        (pin (num 18) (name GND) (type power_in))
        (pin (num 19) (name U0_RXD) (type input))
        (pin (num 20) (name U0_TXD) (type output))
        (pin (num 21) (name P2_9) (type BiDi))
        (pin (num 22) (name P2_13) (type BiDi))
        (pin (num 23) (name P2_8) (type BiDi))
        (pin (num 24) (name SDA) (type BiDi))
        (pin (num 25) (name CLK6) (type output))
        (pin (num 26) (name SCL) (type output))))
    (libpart (lib hackrf_expansion) (part HACKRF_ONE_P28)
      (footprints
        (fp HEADER_11X2_*_254))
      (fields
        (field (name Reference) J)
        (field (name Value) HACKRF_ONE_P28))
      (pins
        (pin (num 1) (name VCC) (type power_out))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name SD_CD) (type BiDi))
        (pin (num 4) (name SD_DAT3) (type BiDi))
        (pin (num 5) (name SD_DAT2) (type BiDi))
        (pin (num 6) (name SD_DAT1) (type BiDi))
        (pin (num 7) (name SD_DAT0) (type BiDi))
        (pin (num 8) (name SD_VOLT0) (type BiDi))
        (pin (num 9) (name SD_CMD) (type BiDi))
        (pin (num 10) (name SD_POW) (type BiDi))
        (pin (num 11) (name SD_CLK) (type BiDi))
        (pin (num 12) (name GND) (type power_in))
        (pin (num 13) (name GCLK2) (type output))
        (pin (num 14) (name GCK1) (type output))
        (pin (num 15) (name B1AUX14) (type BiDi))
        (pin (num 16) (name B1AUX13) (type BiDi))
        (pin (num 17) (name CPLD_TCK) (type output))
        (pin (num 18) (name BANK2F3M2) (type BiDi))
        (pin (num 19) (name CPLD_TDI) (type input))
        (pin (num 20) (name BANK2F3M6) (type BiDi))
        (pin (num 21) (name BANK2F3M12) (type BiDi))
        (pin (num 22) (name BANK2F3M4) (type BiDi))))
    (libpart (lib regulator) (part REGULATOR_SOT23_5)
      (footprints
        (fp IPC_SOT95P280X110-5N))
      (fields
        (field (name Reference) U)
        (field (name Value) REGULATOR_SOT23_5))
      (pins
        (pin (num 1) (name VIN) (type power_in))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name EN) (type input))
        (pin (num 4) (name BP) (type input))
        (pin (num 5) (name VOUT) (type power_out))))
    (libpart (lib hole) (part HOLE1)
      (footprints
        (fp *HOLE*))
      (fields
        (field (name Reference) H)
        (field (name Value) HOLE1))
      (pins
        (pin (num 1) (name ~) (type passive))))
    (libpart (lib sharebrained) (part PORTAPACK_H1)
      (footprints
        (fp portapack_text_300))
      (fields
        (field (name Reference) LOGO)
        (field (name Value) PORTAPACK_H1)))
    (libpart (lib sharebrained) (part SHAREBRAINED)
      (footprints
        (fp sharebrained_text_300))
      (fields
        (field (name Reference) LOGO)
        (field (name Value) SHAREBRAINED)))
    (libpart (lib fiducial) (part FIDUCIAL)
      (footprints
        (fp FIDUCIAL_65MIL))
      (fields
        (field (name Reference) FID)
        (field (name Value) FIDUCIAL))))
  (libraries
    (library (logical lcd_kingtech)
      (uri ../../../../library/kicad/lcd_kingtech.lib))
    (library (logical battery)
      (uri ../../../../library/kicad/battery.lib))
    (library (logical trs_jack)
      (uri ../../../../library/kicad/trs_jack.lib))
    (library (logical mosfet)
      (uri ../../../../library/kicad/mosfet.lib))
    (library (logical microphone)
      (uri ../../../../library/kicad/microphone.lib))
    (library (logical sd)
      (uri ../../../../library/kicad/sd.lib))
    (library (logical altera)
      (uri ../../../../library/kicad/altera.lib))
    (library (logical ck)
      (uri ../../../../library/kicad/ck.lib))
    (library (logical hackrf_expansion)
      (uri ../../../../library/kicad/hackrf_expansion.lib))
    (library (logical passive)
      (uri ../../../../library/kicad/passive.lib))
    (library (logical wolfson)
      (uri ../../../../library/kicad/wolfson.lib))
    (library (logical regulator)
      (uri ../../../../library/kicad/regulator.lib))
    (library (logical hole)
      (uri ../../../../library/kicad/hole.lib))
    (library (logical fiducial)
      (uri ../../../../library/kicad/fiducial.lib))
    (library (logical sharebrained)
      (uri ../../../../library/kicad/sharebrained.lib)))
  (nets
    (net (code 1) (name /hackrf_if/LCD_BACKLIGHT)
      (node (ref U3) (pin 4))
      (node (ref Q1) (pin 1))
      (node (ref R20) (pin 2)))
    (net (code 2) (name /hackrf_if/LCD_RESET#)
      (node (ref U3) (pin 38))
      (node (ref R19) (pin 1))
      (node (ref J3) (pin 5)))
    (net (code 3) (name /hackrf_if/LCD_RS)
      (node (ref U3) (pin 43))
      (node (ref J3) (pin 6)))
    (net (code 4) (name /hackrf_if/LCD_RD#)
      (node (ref U3) (pin 44))
      (node (ref J3) (pin 7)))
    (net (code 5) (name /audio/I2S0_TX_SDA)
      (node (ref RP1) (pin 1))
      (node (ref P22) (pin 13)))
    (net (code 6) (name /audio/I2S0_WS)
      (node (ref P22) (pin 15))
      (node (ref RP1) (pin 2)))
    (net (code 7) (name /audio/I2S0_MCLK)
      (node (ref RP1) (pin 4))
      (node (ref P22) (pin 17)))
    (net (code 8) (name /audio/I2S0_SCK)
      (node (ref P22) (pin 16))
      (node (ref RP1) (pin 3)))
    (net (code 9) (name /audio/SDA)
      (node (ref P22) (pin 24))
      (node (ref U1) (pin 23)))
    (net (code 10) (name /audio/SCL)
      (node (ref U1) (pin 24))
      (node (ref P22) (pin 26)))
    (net (code 11) (name /hackrf_if/SD_CD)
      (node (ref J2) (pin B))
      (node (ref P28) (pin 3)))
    (net (code 12) (name /hackrf_if/SD_DAT2)
      (node (ref P28) (pin 5))
      (node (ref J2) (pin 1)))
    (net (code 13) (name /hackrf_if/SD_DAT0)
      (node (ref P28) (pin 7))
      (node (ref J2) (pin 7)))
    (net (code 14) (name /hackrf_if/SD_CMD)
      (node (ref P28) (pin 9))
      (node (ref J2) (pin 3)))
    (net (code 15) (name /hackrf_if/SD_CLK)
      (node (ref P28) (pin 11))
      (node (ref J2) (pin 5)))
    (net (code 16) (name /hackrf_if/SD_DAT3)
      (node (ref J2) (pin 2))
      (node (ref P28) (pin 4)))
    (net (code 17) (name /hackrf_if/SD_DAT1)
      (node (ref P28) (pin 6))
      (node (ref J2) (pin 8)))
    (net (code 18) (name /audio/I2S0_RX_SDA)
      (node (ref U1) (pin 6))
      (node (ref R22) (pin 2)))
    (net (code 19) (name /hackrf_if/LCD_WR#)
      (node (ref J3) (pin 10))
      (node (ref U3) (pin 45)))
    (net (code 20) (name /hackrf_if/LCD_TE)
      (node (ref U3) (pin 63))
      (node (ref J3) (pin 34)))
    (net (code 21) (name /hackrf_if/TP_U)
      (node (ref P20) (pin 20))
      (node (ref U3) (pin 3))
      (node (ref J3) (pin 40)))
    (net (code 22) (name /hackrf_if/TP_R)
      (node (ref J3) (pin 37))
      (node (ref U3) (pin 64))
      (node (ref P20) (pin 14)))
    (net (code 23) (name /hackrf_if/TP_D)
      (node (ref P20) (pin 16))
      (node (ref U3) (pin 1))
      (node (ref J3) (pin 38)))
    (net (code 24) (name /hackrf_if/TP_L)
      (node (ref U3) (pin 2))
      (node (ref J3) (pin 39))
      (node (ref P20) (pin 18)))
    (net (code 25) (name /hackrf_if/SW_U)
      (node (ref U3) (pin 25))
      (node (ref SW1) (pin S4)))
    (net (code 26) (name /hackrf_if/SW_R)
      (node (ref SW1) (pin S3))
      (node (ref U3) (pin 9)))
    (net (code 27) (name /hackrf_if/SW_D)
      (node (ref U3) (pin 10))
      (node (ref SW1) (pin S2)))
    (net (code 28) (name /hackrf_if/SW_L)
      (node (ref SW1) (pin S5))
      (node (ref U3) (pin 28)))
    (net (code 29) (name /hackrf_if/SW_ROT_A)
      (node (ref U3) (pin 11))
      (node (ref SW1) (pin A)))
    (net (code 30) (name /hackrf_if/SW_ROT_B)
      (node (ref U3) (pin 12))
      (node (ref SW1) (pin B)))
    (net (code 31) (name /hackrf_if/SW_SEL)
      (node (ref SW1) (pin S1))
      (node (ref U3) (pin 13)))
    (net (code 32) (name GND)
      (node (ref H5) (pin 1))
      (node (ref H4) (pin 1))
      (node (ref H3) (pin 1))
      (node (ref H2) (pin 1))
      (node (ref J2) (pin A))
      (node (ref H1) (pin 1))
      (node (ref J2) (pin SH))
      (node (ref C9) (pin 2))
      (node (ref C7) (pin 2))
      (node (ref C12) (pin 2))
      (node (ref C8) (pin 2))
      (node (ref J3) (pin 14))
      (node (ref L10) (pin 2))
      (node (ref J3) (pin 15))
      (node (ref L1) (pin 2))
      (node (ref J3) (pin 35))
      (node (ref J3) (pin 16))
      (node (ref R8) (pin 1))
      (node (ref J3) (pin 17))
      (node (ref R9) (pin 2))
      (node (ref C15) (pin 2))
      (node (ref C13) (pin 2))
      (node (ref C11) (pin 2))
      (node (ref U3) (pin 65))
      (node (ref C2) (pin 2))
      (node (ref J3) (pin 12))
      (node (ref C5) (pin 2))
      (node (ref C4) (pin 2))
      (node (ref J3) (pin 11))
      (node (ref J3) (pin 9))
      (node (ref J3) (pin 8))
      (node (ref J3) (pin 3))
      (node (ref J3) (pin 13))
      (node (ref U2) (pin 2))
      (node (ref C35) (pin 2))
      (node (ref C33) (pin 2))
      (node (ref C31) (pin 2))
      (node (ref Q1) (pin 2))
      (node (ref P20) (pin 13))
      (node (ref P20) (pin 15))
      (node (ref C40) (pin 2))
      (node (ref C38) (pin 2))
      (node (ref SW1) (pin CB))
      (node (ref SW1) (pin CA))
      (node (ref C29) (pin 2))
      (node (ref C27) (pin 2))
      (node (ref C30) (pin 2))
      (node (ref BT1) (pin 2))
      (node (ref C28) (pin 2))
      (node (ref C37) (pin 2))
      (node (ref C36) (pin 2))
      (node (ref C34) (pin 2))
      (node (ref C32) (pin 2))
      (node (ref C26) (pin 2))
      (node (ref C39) (pin 2))
      (node (ref U1) (pin 15))
      (node (ref C42) (pin 2))
      (node (ref C43) (pin 2))
      (node (ref C3) (pin 2))
      (node (ref J2) (pin 0))
      (node (ref L6) (pin 2))
      (node (ref J2) (pin 6))
      (node (ref J3) (pin SHLD))
      (node (ref R19) (pin 2))
      (node (ref R14) (pin 2))
      (node (ref U1) (pin 11))
      (node (ref U1) (pin 21))
      (node (ref U1) (pin 22))
      (node (ref P22) (pin 18))
      (node (ref P28) (pin 2))
      (node (ref R13) (pin 1))
      (node (ref P28) (pin 12))
      (node (ref C41) (pin 2))
      (node (ref C14) (pin 1))
      (node (ref X1) (pin 2))
      (node (ref R11) (pin 1))
      (node (ref R12) (pin 2))
      (node (ref R20) (pin 1))
      (node (ref P22) (pin 10))
      (node (ref P22) (pin 4))
      (node (ref P20) (pin 19))
      (node (ref C25) (pin 2))
      (node (ref R17) (pin 2))
      (node (ref U1) (pin 28))
      (node (ref C6) (pin 2))
      (node (ref C10) (pin 2))
      (node (ref C23) (pin 2))
      (node (ref C22) (pin 1)))
    (net (code 33) (name "Net-(C24-Pad1)")
      (node (ref C24) (pin 1))
      (node (ref R10) (pin 1)))
    (net (code 34) (name "Net-(L8-Pad2)")
      (node (ref R16) (pin 1))
      (node (ref L8) (pin 2)))
    (net (code 35) (name "Net-(L8-Pad1)")
      (node (ref P3) (pin 3))
      (node (ref L8) (pin 1)))
    (net (code 36) (name "Net-(L7-Pad2)")
      (node (ref R15) (pin 1))
      (node (ref L7) (pin 2)))
    (net (code 37) (name "Net-(L7-Pad1)")
      (node (ref P3) (pin 2))
      (node (ref L7) (pin 1)))
    (net (code 38) (name "Net-(L3-Pad2)")
      (node (ref L3) (pin 2))
      (node (ref P1) (pin 3)))
    (net (code 39) (name "Net-(L3-Pad1)")
      (node (ref L3) (pin 1))
      (node (ref R7) (pin 2)))
    (net (code 40) (name "Net-(L2-Pad2)")
      (node (ref L2) (pin 2))
      (node (ref P1) (pin 2)))
    (net (code 41) (name "Net-(L2-Pad1)")
      (node (ref R6) (pin 2))
      (node (ref L2) (pin 1)))
    (net (code 42) (name /audio/RLINEIN)
      (node (ref U1) (pin 19))
      (node (ref C17) (pin 1)))
    (net (code 43) (name /audio/LLINEIN)
      (node (ref C16) (pin 1))
      (node (ref U1) (pin 20)))
    (net (code 44) (name "Net-(C24-Pad2)")
      (node (ref R17) (pin 1))
      (node (ref X1) (pin 1))
      (node (ref R18) (pin 2))
      (node (ref L9) (pin 2))
      (node (ref C24) (pin 2))
      (node (ref C25) (pin 1)))
    (net (code 45) (name "Net-(L5-Pad1)")
      (node (ref P2) (pin 3))
      (node (ref L5) (pin 1)))
    (net (code 46) (name "Net-(L4-Pad1)")
      (node (ref P2) (pin 2))
      (node (ref L4) (pin 1)))
    (net (code 47) (name "Net-(L6-Pad1)")
      (node (ref P2) (pin 4))
      (node (ref L6) (pin 1)))
    (net (code 48) (name "Net-(L9-Pad1)")
      (node (ref P2) (pin 1))
      (node (ref L9) (pin 1)))
    (net (code 49) (name /audio/LOUT)
      (node (ref C20) (pin 1))
      (node (ref U1) (pin 12)))
    (net (code 50) (name /audio/ROUT)
      (node (ref C21) (pin 1))
      (node (ref U1) (pin 13)))
    (net (code 51) (name "Net-(C18-Pad2)")
      (node (ref C22) (pin 2))
      (node (ref R11) (pin 2))
      (node (ref C18) (pin 2))
      (node (ref L4) (pin 2)))
    (net (code 52) (name "Net-(C19-Pad2)")
      (node (ref L5) (pin 2))
      (node (ref C19) (pin 2))
      (node (ref R12) (pin 1))
      (node (ref C23) (pin 1)))
    (net (code 53) (name "Net-(C21-Pad2)")
      (node (ref R14) (pin 1))
      (node (ref C21) (pin 2))
      (node (ref R16) (pin 2)))
    (net (code 54) (name "Net-(C20-Pad2)")
      (node (ref R15) (pin 2))
      (node (ref C20) (pin 2))
      (node (ref R13) (pin 2)))
    (net (code 55) (name +3.3V)
      (node (ref U1) (pin 8))
      (node (ref C42) (pin 1))
      (node (ref U1) (pin 14))
      (node (ref C43) (pin 1))
      (node (ref U3) (pin 6))
      (node (ref P28) (pin 1))
      (node (ref C7) (pin 1))
      (node (ref C9) (pin 1))
      (node (ref C13) (pin 1))
      (node (ref C11) (pin 1))
      (node (ref C2) (pin 1))
      (node (ref C5) (pin 1))
      (node (ref C4) (pin 1))
      (node (ref J3) (pin 4))
      (node (ref J3) (pin 2))
      (node (ref P20) (pin 3))
      (node (ref C38) (pin 1))
      (node (ref U2) (pin 3))
      (node (ref U2) (pin 1))
      (node (ref C34) (pin 1))
      (node (ref C32) (pin 1))
      (node (ref C26) (pin 1))
      (node (ref U3) (pin 23))
      (node (ref C30) (pin 1))
      (node (ref C27) (pin 1))
      (node (ref C28) (pin 1))
      (node (ref P22) (pin 11))
      (node (ref U1) (pin 1))
      (node (ref U1) (pin 27))
      (node (ref J2) (pin 4))
      (node (ref C3) (pin 1)))
    (net (code 56) (name "Net-(P2-Pad6)")
      (node (ref P2) (pin 6)))
    (net (code 57) (name "Net-(P2-Pad5)")
      (node (ref P2) (pin 5)))
    (net (code 58) (name "Net-(C14-Pad2)")
      (node (ref R6) (pin 1))
      (node (ref R8) (pin 2))
      (node (ref C14) (pin 2))
      (node (ref C16) (pin 2)))
    (net (code 59) (name "Net-(C15-Pad1)")
      (node (ref C15) (pin 1))
      (node (ref R7) (pin 1))
      (node (ref C17) (pin 2))
      (node (ref R9) (pin 1)))
    (net (code 60) (name "Net-(L1-Pad1)")
      (node (ref L1) (pin 1))
      (node (ref P1) (pin 1)))
    (net (code 61) (name "Net-(L10-Pad1)")
      (node (ref P3) (pin 1))
      (node (ref L10) (pin 1)))
    (net (code 62) (name "Net-(U1-Pad2)")
      (node (ref U1) (pin 2)))
    (net (code 63) (name "Net-(U1-Pad26)")
      (node (ref U1) (pin 26)))
    (net (code 64) (name /audio/RHPOUT)
      (node (ref U1) (pin 10))
      (node (ref C19) (pin 1)))
    (net (code 65) (name /audio/LHPOUT)
      (node (ref C18) (pin 1))
      (node (ref U1) (pin 9)))
    (net (code 66) (name /audio/MICIN)
      (node (ref R10) (pin 2))
      (node (ref U1) (pin 18)))
    (net (code 67) (name /audio/MICBIAS)
      (node (ref C10) (pin 1))
      (node (ref R18) (pin 1))
      (node (ref U1) (pin 17))
      (node (ref C12) (pin 1)))
    (net (code 68) (name /audio/VMID)
      (node (ref U1) (pin 16))
      (node (ref C6) (pin 1))
      (node (ref C8) (pin 1)))
    (net (code 69) (name /audio/I2S0_WS_R)
      (node (ref U1) (pin 5))
      (node (ref U1) (pin 7))
      (node (ref RP1) (pin 7)))
    (net (code 70) (name /audio/I2S0_MCLK_R)
      (node (ref U1) (pin 25))
      (node (ref RP1) (pin 5)))
    (net (code 71) (name /audio/I2S0_TX_SDA_R)
      (node (ref RP1) (pin 8))
      (node (ref U1) (pin 4)))
    (net (code 72) (name /audio/I2S0_SCK_R)
      (node (ref U1) (pin 3))
      (node (ref RP1) (pin 6)))
    (net (code 73) (name /hackrf_if/CPLD_TCK)
      (node (ref U3) (pin 16))
      (node (ref P28) (pin 17)))
    (net (code 74) (name "Net-(C39-Pad1)")
      (node (ref U2) (pin 4))
      (node (ref C39) (pin 1)))
    (net (code 75) (name /hackrf_if/P1_5)
      (node (ref P28) (pin 10))
      (node (ref U3) (pin 17)))
    (net (code 76) (name "Net-(U3-Pad37)")
      (node (ref U3) (pin 37)))
    (net (code 77) (name /hackrf_if/P2_1_R)
      (node (ref RP4) (pin 8))
      (node (ref U3) (pin 33)))
    (net (code 78) (name "Net-(U3-Pad35)")
      (node (ref U3) (pin 35)))
    (net (code 79) (name "Net-(U3-Pad36)")
      (node (ref U3) (pin 36)))
    (net (code 80) (name /hackrf_if/P2_0_R)
      (node (ref U3) (pin 32))
      (node (ref R3) (pin 1)))
    (net (code 81) (name /hackrf_if/GPIO3_8)
      (node (ref P20) (pin 5))
      (node (ref RP7) (pin 3)))
    (net (code 82) (name /hackrf_if/GPIO3_9)
      (node (ref P20) (pin 6))
      (node (ref RP7) (pin 4)))
    (net (code 83) (name /hackrf_if/GPIO3_10)
      (node (ref RP7) (pin 2))
      (node (ref P20) (pin 7)))
    (net (code 84) (name /hackrf_if/GPIO3_11)
      (node (ref RP7) (pin 1))
      (node (ref P20) (pin 8)))
    (net (code 85) (name /hackrf_if/GPIO3_12)
      (node (ref RP6) (pin 3))
      (node (ref P20) (pin 9)))
    (net (code 86) (name /hackrf_if/GPIO3_13)
      (node (ref P20) (pin 10))
      (node (ref RP6) (pin 4)))
    (net (code 87) (name /hackrf_if/GPIO3_14)
      (node (ref RP6) (pin 2))
      (node (ref P20) (pin 11)))
    (net (code 88) (name /hackrf_if/GPIO3_15)
      (node (ref RP6) (pin 1))
      (node (ref P20) (pin 12)))
    (net (code 89) (name /hackrf_if/P2_13)
      (node (ref P22) (pin 22))
      (node (ref RP4) (pin 4)))
    (net (code 90) (name /hackrf_if/P1_8)
      (node (ref P28) (pin 8))
      (node (ref U3) (pin 14)))
    (net (code 91) (name /hackrf_if/RESET#)
      (node (ref P22) (pin 3))
      (node (ref U3) (pin 29)))
    (net (code 92) (name /hackrf_if/P2_4_R)
      (node (ref U3) (pin 30))
      (node (ref R1) (pin 1)))
    (net (code 93) (name /hackrf_if/CPLD_TDI)
      (node (ref P28) (pin 19))
      (node (ref R22) (pin 1))
      (node (ref U3) (pin 15)))
    (net (code 94) (name /hackrf_if/P2_9)
      (node (ref RP4) (pin 3))
      (node (ref P22) (pin 21)))
    (net (code 95) (name /hackrf_if/P2_8_R)
      (node (ref U3) (pin 34))
      (node (ref RP4) (pin 7)))
    (net (code 96) (name "Net-(U3-Pad7)")
      (node (ref U3) (pin 7)))
    (net (code 97) (name "Net-(U3-Pad5)")
      (node (ref U3) (pin 5)))
    (net (code 98) (name /hackrf_if/P2_8)
      (node (ref P22) (pin 23))
      (node (ref RP4) (pin 2)))
    (net (code 99) (name /hackrf_if/VBAT)
      (node (ref C41) (pin 1))
      (node (ref BT1) (pin 1))
      (node (ref P20) (pin 1)))
    (net (code 100) (name /hackrf_if/P2_3_R)
      (node (ref R2) (pin 1))
      (node (ref U3) (pin 31)))
    (net (code 101) (name +1.8V)
      (node (ref C35) (pin 1))
      (node (ref C31) (pin 1))
      (node (ref C29) (pin 1))
      (node (ref U2) (pin 5))
      (node (ref C40) (pin 1))
      (node (ref U3) (pin 57))
      (node (ref U3) (pin 39))
      (node (ref J3) (pin 36))
      (node (ref U3) (pin 41))
      (node (ref C33) (pin 1))
      (node (ref C37) (pin 1))
      (node (ref C36) (pin 1))
      (node (ref U3) (pin 8)))
    (net (code 102) (name /hackrf_if/GPIO3_15_R)
      (node (ref U3) (pin 18))
      (node (ref RP6) (pin 8)))
    (net (code 103) (name /hackrf_if/GPIO3_14_R)
      (node (ref U3) (pin 19))
      (node (ref RP6) (pin 7)))
    (net (code 104) (name /hackrf_if/GPIO3_12_R)
      (node (ref U3) (pin 20))
      (node (ref RP6) (pin 6)))
    (net (code 105) (name /hackrf_if/GPIO3_13_R)
      (node (ref U3) (pin 21))
      (node (ref RP6) (pin 5)))
    (net (code 106) (name /hackrf_if/GPIO3_11_R)
      (node (ref U3) (pin 22))
      (node (ref RP7) (pin 8)))
    (net (code 107) (name /hackrf_if/GPIO3_10_R)
      (node (ref RP7) (pin 7))
      (node (ref U3) (pin 24)))
    (net (code 108) (name /hackrf_if/GPIO3_8_R)
      (node (ref U3) (pin 26))
      (node (ref RP7) (pin 6)))
    (net (code 109) (name /hackrf_if/GPIO3_9_R)
      (node (ref U3) (pin 27))
      (node (ref RP7) (pin 5)))
    (net (code 110) (name /hackrf_if/P2_13_R)
      (node (ref RP4) (pin 5))
      (node (ref U3) (pin 42)))
    (net (code 111) (name /hackrf_if/P2_9_R)
      (node (ref RP4) (pin 6))
      (node (ref U3) (pin 40)))
    (net (code 112) (name /hackrf_if/P2_4)
      (node (ref R1) (pin 2))
      (node (ref P22) (pin 5)))
    (net (code 113) (name /hackrf_if/P2_1)
      (node (ref RP4) (pin 1))
      (node (ref P22) (pin 19)))
    (net (code 114) (name /hackrf_if/P2_0)
      (node (ref P22) (pin 20))
      (node (ref R3) (pin 2)))
    (net (code 115) (name "Net-(P20-Pad22)")
      (node (ref P20) (pin 22)))
    (net (code 116) (name "Net-(P20-Pad21)")
      (node (ref P20) (pin 21)))
    (net (code 117) (name "Net-(P20-Pad4)")
      (node (ref P20) (pin 4)))
    (net (code 118) (name "Net-(P20-Pad2)")
      (node (ref P20) (pin 2)))
    (net (code 119) (name "Net-(P22-Pad14)")
      (node (ref P22) (pin 14)))
    (net (code 120) (name "Net-(P22-Pad12)")
      (node (ref P22) (pin 12)))
    (net (code 121) (name "Net-(P22-Pad25)")
      (node (ref P22) (pin 25)))
    (net (code 122) (name "Net-(P22-Pad9)")
      (node (ref P22) (pin 9)))
    (net (code 123) (name "Net-(P22-Pad8)")
      (node (ref P22) (pin 8)))
    (net (code 124) (name "Net-(P22-Pad7)")
      (node (ref P22) (pin 7)))
    (net (code 125) (name /hackrf_if/P2_3)
      (node (ref R2) (pin 2))
      (node (ref P22) (pin 6)))
    (net (code 126) (name "Net-(P22-Pad2)")
      (node (ref P22) (pin 2)))
    (net (code 127) (name "Net-(P22-Pad1)")
      (node (ref P22) (pin 1)))
    (net (code 128) (name "Net-(P20-Pad17)")
      (node (ref P20) (pin 17)))
    (net (code 129) (name "Net-(P28-Pad13)")
      (node (ref P28) (pin 13)))
    (net (code 130) (name "Net-(P28-Pad14)")
      (node (ref P28) (pin 14)))
    (net (code 131) (name "Net-(P28-Pad16)")
      (node (ref P28) (pin 16)))
    (net (code 132) (name "Net-(P28-Pad15)")
      (node (ref P28) (pin 15)))
    (net (code 133) (name "Net-(P28-Pad21)")
      (node (ref P28) (pin 21)))
    (net (code 134) (name "Net-(P28-Pad22)")
      (node (ref P28) (pin 22)))
    (net (code 135) (name "Net-(P28-Pad20)")
      (node (ref P28) (pin 20)))
    (net (code 136) (name "Net-(P28-Pad18)")
      (node (ref P28) (pin 18)))
    (net (code 137) (name "Net-(J3-Pad1)")
      (node (ref Q1) (pin 3))
      (node (ref J3) (pin 1)))
    (net (code 138) (name /hackrf_if/LCD_DB4)
      (node (ref U3) (pin 58))
      (node (ref J3) (pin 29)))
    (net (code 139) (name /hackrf_if/LCD_DB5)
      (node (ref U3) (pin 56))
      (node (ref J3) (pin 28)))
    (net (code 140) (name /hackrf_if/LCD_DB6)
      (node (ref J3) (pin 27))
      (node (ref U3) (pin 55)))
    (net (code 141) (name /hackrf_if/LCD_DB7)
      (node (ref J3) (pin 26))
      (node (ref U3) (pin 54)))
    (net (code 142) (name /hackrf_if/LCD_DB8)
      (node (ref J3) (pin 25))
      (node (ref U3) (pin 53)))
    (net (code 143) (name /hackrf_if/LCD_DB9)
      (node (ref J3) (pin 24))
      (node (ref U3) (pin 52)))
    (net (code 144) (name /hackrf_if/LCD_DB10)
      (node (ref J3) (pin 23))
      (node (ref U3) (pin 51)))
    (net (code 145) (name /hackrf_if/LCD_DB11)
      (node (ref J3) (pin 22))
      (node (ref U3) (pin 50)))
    (net (code 146) (name /hackrf_if/LCD_DB12)
      (node (ref J3) (pin 21))
      (node (ref U3) (pin 49)))
    (net (code 147) (name /hackrf_if/LCD_DB13)
      (node (ref J3) (pin 20))
      (node (ref U3) (pin 48)))
    (net (code 148) (name /hackrf_if/LCD_DB14)
      (node (ref U3) (pin 47))
      (node (ref J3) (pin 19)))
    (net (code 149) (name /hackrf_if/LCD_DB15)
      (node (ref U3) (pin 46))
      (node (ref J3) (pin 18)))
    (net (code 150) (name /hackrf_if/LCD_DB0)
      (node (ref U3) (pin 62))
      (node (ref J3) (pin 33)))
    (net (code 151) (name /hackrf_if/LCD_DB1)
      (node (ref U3) (pin 61))
      (node (ref J3) (pin 32)))
    (net (code 152) (name /hackrf_if/LCD_DB2)
      (node (ref J3) (pin 31))
      (node (ref U3) (pin 60)))
    (net (code 153) (name /hackrf_if/LCD_DB3)
      (node (ref U3) (pin 59))
      (node (ref J3) (pin 30)))))